;
; This product is covered by one or more of the following patents:
; US6,570,884, US6,115,776, and US6,327,625.
;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Killer%
PnpLockDown = 1
DriverVer   = 06/15/2022,10.060.0615.2022
CatalogFile = e2kw10x64.cat

[Manufacturer]
%Killer%=Killer, NTx86.10.0, NTamd64.10.0

[ControlFlags]
ExcludeFromSelect     = *

[Killer]
;Empty section, so this INF does not support win2000

[Killer.NTx86.10.0]
;Empty section, so this INF does not support win10 x86

[Killer.NTamd64.10.0]

%Killer_LAN_0.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_2502&REV_1F
%Killer_LAN_1.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_2502&SUBSYS_25021A56&REV_1F
%Killer_LAN_2.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_2600&REV_21
%Killer_LAN_3.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_2600&SUBSYS_26001A56&REV_21

[RTL8118AS.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, MSWoLMagPktDisabled.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEDisable.reg, GreenEthEnabled.reg, AdvancedEEEDisable.reg
AddReg          = GigaLite.reg, GPPSWEnabled.reg
AddReg          = RegVlanid.reg
AddReg          = rtk.reg
CopyFiles       = rt640.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8118AS.ndi.NT.HW]
AddReg = MSI.01.AddReg

[MSI.00.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[MSI.01.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1
HKR, "Interrupt Management\Affinity Policy", 0x00000010
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 1
HKR, "Interrupt Management\Affinity Policy", DevicePriority, 0x00010001, 3

[MSI.04.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 4
HKR, "Interrupt Management\Affinity Policy", 0x00000010
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 1
HKR, "Interrupt Management\Affinity Policy", DevicePriority, 0x00010001, 3

[MSI.16.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 16
HKR, "Interrupt Management\Affinity Policy", 0x00000010
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 1
HKR, "Interrupt Management\Affinity Policy", DevicePriority, 0x00010001, 3

[MSI.32.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 32
HKR, "Interrupt Management\Affinity Policy", 0x00000010
HKR, "Interrupt Management\Affinity Policy", DevicePolicy, 0x00010001, 1
HKR, "Interrupt Management\Affinity Policy", DevicePriority, 0x00010001, 3


[RTL8118AS.ndi.NT.Services]
AddService = e2kw10x64, 2, rt640.Service, common.EventLog

[Common.reg]
HKR,,DeviceRemovable,0,"0"

HKR,,HwParaMask,0x00010001,0

HKR,,HwPciOtherFunDevMask,0x00010001,0

HKR,,HwOptimize,0x00010001,0

HKR,,HwMode,0x00010001,0

HKR,,HwOption,0x00010001,0x800000

HKR,,HwWolCrcVal,0x00010001,0

HKR,,LogDisconnectEvent,0,"0"

HKR,,EnableEDT,0,"1"

HKR,,RIACP,0,"0"

HKR,,S5NicKeepOverrideMacAddr,0,"0"

HKR,,S5NicKeepOverrideMacAddrV2,0,"1"

HKR,,PPSW,0,"1"

HKR,,GPPSW,0,"0"

HKR,,S0MgcPkt,0,"0"

HKR,,HwFPSM,0x00010001,0

HKR,,SwIML,0x00010001,0

HKR,,SwIML100,0x00010001,0

HKR,,SwIMLV2,0x00010001,0

HKR,,SwIML100V2,0x00010001,0

HKR,,ENPWMode,0,"0"

HKR,,Diskless,0,"0"

HKR,,DisklessOption,0,"0"

HKR,,TxOptimizeThreshold,0x00010001,0

HKR,,RxOptimizeThreshold,0x00010001,0

HKR,,CFHTime,0x00010001,0

HKR,,LDWTime,0x00010001,0

HKR,,RMPT,0x00010001,0

HKR,,CRSPDThreshold,0x00010001,0

HKR,,ComboPerfAdjust,0,"0"

HKR,,CHNLWTime,0x00010001,0

HKR,,CHNLWCnt,0x00010001,0

HKR,,L1L0sLT,0x00010001,0

HKR,,MRRSize,0x00010001,0

HKR,,TDBSize,0x00010001,0xFFFFFFFF

HKR,,RDBSize,0x00010001,0xFFFFFFFF

HKR,,HwOptionV2,0x00010001,0

HKR,,HwOptionV3,0x00010001,0

HKR,,HwOptionV4,0x00010001,0

HKR,,HwBpMask,0x00010001,0

HKR,,MonitorModeEnabled,0,"0"

HKR,,UCEM,0x00010001,0

HKR,,FactoryMode,0,"0"

HKR,,SwParaMask,0x00010001,0

HKR,Ndi\params\PowerSavingMode,    ParamDesc,  0, %PowerSavingMode%
HKR,Ndi\params\PowerSavingMode,    default,    0, "1"
HKR,Ndi\params\PowerSavingMode,    type,       0, "enum"
HKR,Ndi\params\PowerSavingMode\enum,   "0",    0, %Disabled%
HKR,Ndi\params\PowerSavingMode\enum,   "1",    0, %Enabled%
HKR,,PowerSavingMode,0,"1"

[Speed.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

HKR,Ndi\params\AutoDisableGigabit,       ParamDesc,  0, %AutoDisableGigabit%
HKR,Ndi\params\AutoDisableGigabit,       default,    0, "0"
;HKR,Ndi\params\AutoDisableGigabit,       optional,   0, "1"
HKR,Ndi\params\AutoDisableGigabit,       type,       0, "enum"
HKR,Ndi\params\AutoDisableGigabit\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoDisableGigabit\enum,  "1",        0, %BatteryRe-Link%
HKR,Ndi\params\AutoDisableGigabit\enum,  "2",        0, %AcBatteryRe-Link%
HKR,,AutoDisableGigabit,0,"0"

[SpeedAuto.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[SpeedHideAuto.reg]
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[Speed1g.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "6"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"6"

HKR,,ForceMode,0,"0"

[Speed10_100.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[SpeedForce100Full.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"4"

HKR,,ForceMode,0,"1"

[Speed2.5G.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2500",     0, %2.5Gb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[DisIntModer100M.reg]
HKR,,SwIML100,0x00010001,0x140

[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,     ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,     type,       0, "edit"
HKR,Ndi\params\NetworkAddress,     default,    0, ""
HKR,Ndi\params\NetworkAddress,     LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,     UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,     Optional,   0, "1"

[flowctrl.reg]
HKR,Ndi\params\*FlowControl,       ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,       default,    0, "3"
HKR,Ndi\params\*FlowControl,       type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "3",        0, %RxTxEnabled%
HKR,,*FlowControl,0,"3"

[flowctrlDisable.reg]
HKR,Ndi\params\*FlowControl,       ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,       default,    0, "0"
HKR,Ndi\params\*FlowControl,       type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "3",        0, %RxTxEnabled%
HKR,,*FlowControl,0,"0"

[PriorityVlanTag.reg]
HKR,Ndi\params\*PriorityVLANTag,    ParamDesc,  0, %PriorityVLAN%
HKR,Ndi\params\*PriorityVLANTag,    default,    0, "3"
HKR,Ndi\params\*PriorityVLANTag,    type,       0, "enum"
HKR,Ndi\params\*PriorityVLANTag\enum,   "0",        0, %PriorityVLANDisabled%
HKR,Ndi\params\*PriorityVLANTag\enum,   "1",        0, %PriorityEnabled%
HKR,Ndi\params\*PriorityVLANTag\enum,   "2",        0, %VLANEnabled%
HKR,Ndi\params\*PriorityVLANTag\enum,   "3",        0, %PriorityVLANEnabled%
HKR,,*PriorityVLANTag,0,"3"

[InterruptModeration.reg]
HKR,Ndi\params\*InterruptModeration,    ParamDesc,  0, %InterruptModeration%
HKR,Ndi\params\*InterruptModeration,    default,    0, "1"
HKR,Ndi\params\*InterruptModeration,    type,       0, "enum"
HKR,Ndi\params\*InterruptModeration\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*InterruptModeration\enum,   "1",        0, %Enabled%
HKR,,*InterruptModeration,0,"1"

[TxRxBuf.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "32"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "8"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "32"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "8"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"128"

[TxRxBuf8125.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "32"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "8"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "512"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "64"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "4096"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "8"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"512"

[Jumboframe.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "4088",     0, %4KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe4k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "4088",     0, %4KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe9k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "4088",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "9014",     0, %9KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe16k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "4088",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "9014",     0, %9KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "16128",    0, %16KBMTU%
HKR,,*JumboPacket,0,"1514"

[JumboNolimit.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "4088",     0, %4KBMTU%
HKR,,*JumboPacket,0,"1514"
HKR,,LimitCbJumboFrame,0,"0"

[Offload.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*LsoV1IPv4,  ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,  default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,  type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadChksum.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

[s5wol.reg]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "1"
;HKR,Ndi\params\S5WakeOnLan,       optional,   0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[s5arpoffload.reg]
HKR,Ndi\params\S5ARPOffload,       ParamDesc,  0, %S5ARPOffload%
HKR,Ndi\params\S5ARPOffload,       default,    0, "1"
;HKR,Ndi\params\S5ARPOffload,       optional,   0, "1"
HKR,Ndi\params\S5ARPOffload,       type,       0, "enum"
HKR,Ndi\params\S5ARPOffload\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5ARPOffload\enum,  "1",        0, %Enabled%
HKR,,S5ARPOffload,0,"1"

[s5arpoffloaddisable.reg]
HKR,Ndi\params\S5ARPOffload,       ParamDesc,  0, %S5ARPOffload%
HKR,Ndi\params\S5ARPOffload,       default,    0, "1"
;HKR,Ndi\params\S5ARPOffload,       optional,   0, "1"
HKR,Ndi\params\S5ARPOffload,       type,       0, "enum"
HKR,Ndi\params\S5ARPOffload\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5ARPOffload\enum,  "1",        0, %Enabled%
HKR,,S5ARPOffload,0,"0"

[s5woldefaultdisable.reg]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "0"
;HKR,Ndi\params\S5WakeOnLan,       optional,   0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"0"

[s5wolhidetype2.reg]
HKR,,S5WakeOnLan,0,"2"

[s5wolhideenable.reg]
HKR,,S5WakeOnLan,0,"1"

[s5wolhidedisable.reg]
HKR,,S5WakeOnLan,0,"0"

[OffloadIpv6Lsov2.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*LsoV2IPv4,  ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,  default,    0, "0"
HKR,Ndi\params\*LsoV2IPv4,  type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"0"

HKR,Ndi\params\*LsoV2IPv6,  ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,  default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,  type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

HKR,Ndi\params\*RSS,    ParamDesc,  0, %RSS%
HKR,Ndi\params\*RSS,    default,    0, "1"
HKR,Ndi\params\*RSS,    type,       0, "enum"
HKR,Ndi\params\*RSS\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*RSS\enum,  "1",        0, %Enabled%
HKR,,*RSS,0,"1"

HKR,Ndi\params\*LsoV1IPv4,  ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,  default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,  type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",       0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",       0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadIpv6Lsov2_8102.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*RSS,    ParamDesc,  0, %RSS%
HKR,Ndi\params\*RSS,    default,    0, "1"
HKR,Ndi\params\*RSS,    type,       0, "enum"
HKR,Ndi\params\*RSS\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*RSS\enum,  "1",        0, %Enabled%
HKR,,*RSS,0,"1"

HKR,Ndi\params\*LsoV2IPv4,  ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,  default,    0, "1"
HKR,Ndi\params\*LsoV2IPv4,  type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"1"

HKR,Ndi\params\*LsoV2IPv6,  ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,  default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,  type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

[AutoCrossoverDet.reg]
HKR,Ndi\params\AutoCrossoverDet,    ParamDesc,  0, %AutoCrossoverDet%
HKR,Ndi\params\AutoCrossoverDet,    default,    0, "0"
;HKR,Ndi\params\AutoCrossoverDet,    optional,   0, "1"
HKR,Ndi\params\AutoCrossoverDet,    type,       0, "enum"
HKR,Ndi\params\AutoCrossoverDet\enum,   "0",        0, %Disabled%
HKR,Ndi\params\AutoCrossoverDet\enum,   "1",        0, %Enabled%
HKR,,AutoCrossoverDet,0,"0"

[powersavingautopcie.reg]
HKR,Ndi\params\AutoLinkDownPcieMacOff,       ParamDesc,  0, %AutoLinkDownPcieMacOff%
HKR,Ndi\params\AutoLinkDownPcieMacOff,       default,    0, "0"
;HKR,Ndi\params\AutoLinkDownPcieMacOff,       optional,   0, "1"
HKR,Ndi\params\AutoLinkDownPcieMacOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPcieMacOff,0,"0"

[SelectiveSuspend.reg]
HKR,Ndi\params\*SelectiveSuspend,         ParamDesc,  0, %SelectiveSuspend%
HKR,Ndi\params\*SelectiveSuspend,         default,    0, "1"
HKR,Ndi\params\*SelectiveSuspend,         type,       0, "enum"
HKR,Ndi\params\*SelectiveSuspend\enum,    "0",        0, %Disabled%
HKR,Ndi\params\*SelectiveSuspend\enum,    "1",        0, %Enabled%
HKR,,*SelectiveSuspend,0,"1"

HKR,Ndi\params\*SSIdleTimeout,      ParamDesc,  0, %SSIdleTimeout%
HKR,Ndi\params\*SSIdleTimeout,      type,       0, "int"
HKR,Ndi\params\*SSIdleTimeout,      default,    0, "50"
HKR,Ndi\Params\*SSIdleTimeout,      Min,        0, "1"
HKR,Ndi\Params\*SSIdleTimeout,      Max,        0, "60"
HKR,Ndi\Params\*SSIdleTimeout,      Step,       0, "1"
HKR,Ndi\Params\*SSIdleTimeout,      Base,       0, "10"
HKR,,*SSIdleTimeout,0,"50"

[AIPSSelectiveSuspend.reg]
HKR,Ndi\params\*SelectiveSuspend,         ParamDesc,  0, %AIPSSelectiveSuspend%
HKR,Ndi\params\*SelectiveSuspend,         default,    0, "0"
HKR,Ndi\params\*SelectiveSuspend,         type,       0, "enum"
HKR,Ndi\params\*SelectiveSuspend\enum,    "0",        0, %Disabled%
HKR,Ndi\params\*SelectiveSuspend\enum,    "1",        0, %Enabled%
HKR,,*SelectiveSuspend,0,"0"

HKR,Ndi\params\*SSIdleTimeout,      ParamDesc,  0, %AIPSSSIdleTimeout%
HKR,Ndi\params\*SSIdleTimeout,      type,       0, "int"
HKR,Ndi\params\*SSIdleTimeout,      default,    0, "50"
HKR,Ndi\Params\*SSIdleTimeout,      Min,        0, "1"
HKR,Ndi\Params\*SSIdleTimeout,      Max,        0, "60"
HKR,Ndi\Params\*SSIdleTimeout,      Step,       0, "1"
HKR,Ndi\Params\*SSIdleTimeout,      Base,       0, "10"
HKR,,*SSIdleTimeout,0,"50"

[WolShutdownLinkSpeed.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,    ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,    default,    0, "0"
;HKR,Ndi\params\WolShutdownLinkSpeed,    optional,   0, "1"
HKR,Ndi\params\WolShutdownLinkSpeed,    type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "0",    0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "1",    0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"0"

[WolS5LinkSpeedNotSpdDown.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,    ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,    default,    0, "2"
;HKR,Ndi\params\WolShutdownLinkSpeed,    optional,   0, "1"
HKR,Ndi\params\WolShutdownLinkSpeed,    type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "0",    0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "1",    0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolS5LinkSpeedForce1g.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,    ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,    default,    0, "2"
;HKR,Ndi\params\WolShutdownLinkSpeed,    optional,   0, "1"
HKR,Ndi\params\WolShutdownLinkSpeed,    type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolS5LinkSpeedHideNotSpdDown.reg]
HKR,,WolShutdownLinkSpeed,0,"2"

[wolptnmagic.reg]
HKR,Ndi\params\*WakeOnPattern,  ParamDesc,  0, %WakeOnPtn%
HKR,Ndi\params\*WakeOnPattern,  default,    0, "1"
HKR,Ndi\params\*WakeOnPattern,  type,       0, "enum"
HKR,Ndi\params\*WakeOnPattern\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnPattern\enum,   "1",        0, %Enabled%
HKR,,*WakeOnPattern,0,"1"

HKR,Ndi\params\*WakeOnMagicPacket,  ParamDesc,  0, %WakeOnMagPkt%
HKR,Ndi\params\*WakeOnMagicPacket,  default,    0, "1"
HKR,Ndi\params\*WakeOnMagicPacket,  type,       0, "enum"
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "1",        0, %Enabled%
HKR,,*WakeOnMagicPacket,0,"1"

[wolptnmagicDisable.reg]
HKR,Ndi\params\*WakeOnPattern,  ParamDesc,  0, %WakeOnPtn%
HKR,Ndi\params\*WakeOnPattern,  default,    0, "0"
HKR,Ndi\params\*WakeOnPattern,  type,       0, "enum"
HKR,Ndi\params\*WakeOnPattern\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnPattern\enum,   "1",        0, %Enabled%
HKR,,*WakeOnPattern,0,"0"

HKR,Ndi\params\*WakeOnMagicPacket,  ParamDesc,  0, %WakeOnMagPkt%
HKR,Ndi\params\*WakeOnMagicPacket,  default,    0, "0"
HKR,Ndi\params\*WakeOnMagicPacket,  type,       0, "enum"
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "1",        0, %Enabled%
HKR,,*WakeOnMagicPacket,0,"0"

[MSWoLMagPktEnabled.reg]
HKR,Ndi\params\*ModernStandbyWoLMagicPacket,  ParamDesc,  0, %MSWoLMagPkt%
HKR,Ndi\params\*ModernStandbyWoLMagicPacket,  default,    0, "0"
HKR,Ndi\params\*ModernStandbyWoLMagicPacket,  type,       0, "enum"
HKR,Ndi\params\*ModernStandbyWoLMagicPacket\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*ModernStandbyWoLMagicPacket\enum,   "1",        0, %Enabled%
HKR,,*ModernStandbyWoLMagicPacket,0,"1"

[MSWoLMagPktDisabled.reg]
HKR,Ndi\params\*ModernStandbyWoLMagicPacket,  ParamDesc,  0, %MSWoLMagPkt%
HKR,Ndi\params\*ModernStandbyWoLMagicPacket,  default,    0, "0"
HKR,Ndi\params\*ModernStandbyWoLMagicPacket,  type,       0, "enum"
HKR,Ndi\params\*ModernStandbyWoLMagicPacket\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*ModernStandbyWoLMagicPacket\enum,   "1",        0, %Enabled%
HKR,,*ModernStandbyWoLMagicPacket,0,"0"

[GreenEthEnabled.reg]
HKR, Ndi\params\EnableGreenEthernet,        ParamDesc,  0, %GreenEthernet%
;HKR, Ndi\params\EnableGreenEthernet,        optional,   0, "1"
HKR, Ndi\params\EnableGreenEthernet,        type,       0, "enum"
HKR, Ndi\params\EnableGreenEthernet,        default,    0, "1"
HKR, Ndi\params\EnableGreenEthernet\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EnableGreenEthernet\enum,   "1",        0, %Enabled%
HKR,,EnableGreenEthernet,0,"1"

[GreenEthDisabled.reg]
HKR, Ndi\params\EnableGreenEthernet,        ParamDesc,  0, %GreenEthernet%
;HKR, Ndi\params\EnableGreenEthernet,        optional,   0, "1"
HKR, Ndi\params\EnableGreenEthernet,        type,       0, "enum"
HKR, Ndi\params\EnableGreenEthernet,        default,    0, "0"
HKR, Ndi\params\EnableGreenEthernet\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EnableGreenEthernet\enum,   "1",        0, %Enabled%
HKR,,EnableGreenEthernet,0,"0"

[ArpNsProtOffload.reg]
HKR,Ndi\params\*PMARPOffload,       ParamDesc,  0, %ArpOffload%
HKR,Ndi\params\*PMARPOffload,       default,    0, "1"
HKR,Ndi\params\*PMARPOffload,       type,       0, "enum"
HKR,Ndi\params\*PMARPOffload\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*PMARPOffload\enum,  "1",        0, %Enabled%
HKR,,*PMARPOffload,0,"1"

HKR,Ndi\params\*PMNSOffload,        ParamDesc,  0, %NsOffload%
HKR,Ndi\params\*PMNSOffload,        default,    0, "1"
HKR,Ndi\params\*PMNSOffload,        type,       0, "enum"
HKR,Ndi\params\*PMNSOffload\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*PMNSOffload\enum,   "1",        0, %Enabled%
HKR,,*PMNSOffload,0,"1"

[EEEMaxSupportSpeed2500_1000.reg]
HKR,Ndi\params\EEEMaxSupportSpeed,       ParamDesc,  0, %EEEMaxSupportSpeed%
HKR,Ndi\params\EEEMaxSupportSpeed,       default,    0, "1000"
HKR,Ndi\params\EEEMaxSupportSpeed,       type,       0, "enum"
HKR,Ndi\params\EEEMaxSupportSpeed\enum,  "10",       0, %10Mb-Full-Duplex%
HKR,Ndi\params\EEEMaxSupportSpeed\enum,  "100",      0, %100Mb-Full-Duplex%
HKR,Ndi\params\EEEMaxSupportSpeed\enum,  "1000",     0, %1000Mb-Full-Duplex%
HKR,Ndi\params\EEEMaxSupportSpeed\enum,  "2500",     0, %2.5Gb-Full-Duplex%
HKR,,EEEMaxSupportSpeed,0,"1000"

[EEE.reg]
HKR, Ndi\params\*EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\*EEE,        type,       0, "enum"
HKR, Ndi\params\*EEE,        default,    0, "1"
HKR, Ndi\params\*EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\*EEE\enum,   "1",        0, %Enabled%
HKR,,*EEE,0,"1"

[EEEEnable.reg]
HKR, Ndi\params\*EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\*EEE,        type,       0, "enum"
HKR, Ndi\params\*EEE,        default,    0, "1"
HKR, Ndi\params\*EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\*EEE\enum,   "1",        0, %Enabled%
HKR,,*EEE,0,"1"

[EEEDisable.reg]
HKR, Ndi\params\*EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\*EEE,        type,       0, "enum"
HKR, Ndi\params\*EEE,        default,    0, "0"
HKR, Ndi\params\*EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\*EEE\enum,   "1",        0, %Enabled%
HKR,,*EEE,0,"0"

[AdvancedEEEEnable.reg]
HKR, Ndi\params\AdvancedEEE,        ParamDesc,  0, %AdvancedEEE%
;HKR, Ndi\params\AdvancedEEE,        optional,   0, "1"
HKR, Ndi\params\AdvancedEEE,        type,       0, "enum"
HKR, Ndi\params\AdvancedEEE,        default,    0, "1"
HKR, Ndi\params\AdvancedEEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\AdvancedEEE\enum,   "1",        0, %Enabled%
HKR,,AdvancedEEE,0,"1"

[AdvancedEEEDisable.reg]
HKR, Ndi\params\AdvancedEEE,        ParamDesc,  0, %AdvancedEEE%
;HKR, Ndi\params\AdvancedEEE,        optional,   0, "1"
HKR, Ndi\params\AdvancedEEE,        type,       0, "enum"
HKR, Ndi\params\AdvancedEEE,        default,    0, "0"
HKR, Ndi\params\AdvancedEEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\AdvancedEEE\enum,   "1",        0, %Enabled%
HKR,,AdvancedEEE,0,"0"

[GigaLite.reg]
HKR, Ndi\params\GigaLite,        ParamDesc,  0, %GigaLite%
;HKR, Ndi\params\GigaLite,        optional,   0, "1"
HKR, Ndi\params\GigaLite,        type,       0, "enum"
HKR, Ndi\params\GigaLite,        default,    0, "1"
HKR, Ndi\params\GigaLite\enum,   "0",        0, %Disabled%
HKR, Ndi\params\GigaLite\enum,   "1",        0, %Enabled%
HKR,,GigaLite,0,"1"

[GigaLiteDisable.reg]
HKR, Ndi\params\GigaLite,        ParamDesc,  0, %GigaLite%
;HKR, Ndi\params\GigaLite,        optional,   0, "1"
HKR, Ndi\params\GigaLite,        type,       0, "enum"
HKR, Ndi\params\GigaLite,        default,    0, "1"
HKR, Ndi\params\GigaLite\enum,   "0",        0, %Disabled%
HKR, Ndi\params\GigaLite\enum,   "1",        0, %Enabled%
HKR,,GigaLite,0,"0"

[HDSplit.reg]
HKR,Ndi\params\*HeaderDataSplit,    ParamDesc,  0, %HDSplit%
HKR,Ndi\params\*HeaderDataSplit,    default,    0, "0"
HKR,Ndi\params\*HeaderDataSplit,    type,       0, "enum"
HKR,Ndi\params\*HeaderDataSplit\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*HeaderDataSplit\enum,   "1",        0, %Enabled%
HKR,,*HeaderDataSplit,0,"0"

[WakeOnLinkUp.reg]
HKR,Ndi\params\WakeOnLinkUp,       ParamDesc,  0, %WakeOnLinkUp%
HKR,Ndi\params\WakeOnLinkUp,       default,    0, "1"
;HKR,Ndi\params\WakeOnLinkUp,       optional,   0, "1"
HKR,Ndi\params\WakeOnLinkUp,       type,       0, "enum"
HKR,Ndi\params\WakeOnLinkUp\enum,  "0",        0, %Disabled%
HKR,Ndi\params\WakeOnLinkUp\enum,  "1",        0, %Enabled%
HKR,,WakeOnLinkUp,0,"1"

[WakeOnLinkChgEnable.reg]
HKR, Ndi\params\WakeOnLinkChg,        ParamDesc,  0, %WakeOnLinkChg%
;HKR, Ndi\params\WakeOnLinkChg,        optional,   0, "1"
HKR, Ndi\params\WakeOnLinkChg,        type,       0, "enum"
HKR, Ndi\params\WakeOnLinkChg,        default,    0, "1"
HKR, Ndi\params\WakeOnLinkChg\enum,   "0",        0, %Disabled%
HKR, Ndi\params\WakeOnLinkChg\enum,   "1",        0, %Enabled%
HKR,,WakeOnLinkChg,0,"1"

[Rss2Q.reg]
HKR, Ndi\Params\*NumRssQueues,         ParamDesc, 0, %NumRssQueues%
HKR, Ndi\Params\*NumRssQueues,         default,   0, "2"
HKR, Ndi\Params\*NumRssQueues,         type,      0, "enum"
HKR, Ndi\Params\*NumRssQueues\Enum,    "1",       0, %1Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,    "2",       0, %2Queue%
HKR,,*NumRssQueues,0,"2"

[Rss4Q.reg]
HKR, Ndi\Params\*NumRssQueues,         ParamDesc, 0, %NumRssQueues%
HKR, Ndi\Params\*NumRssQueues,         default,   0, "4"
HKR, Ndi\Params\*NumRssQueues,         type,      0, "enum"
HKR, Ndi\Params\*NumRssQueues\Enum,    "1",       0, %1Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,    "2",       0, %2Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,    "4",       0, %4Queue%
HKR,,*NumRssQueues,0,"4"

[Rss4Q_2Q.reg]
HKR, Ndi\Params\*NumRssQueues,         ParamDesc, 0, %NumRssQueues%
HKR, Ndi\Params\*NumRssQueues,         default,   0, "2"
HKR, Ndi\Params\*NumRssQueues,         type,      0, "enum"
HKR, Ndi\Params\*NumRssQueues\Enum,    "1",       0, %1Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,    "2",       0, %2Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,    "4",       0, %4Queue%
HKR,,*NumRssQueues,0,"2"

[RegVlanid.reg]
HKR, Ndi\params\RegVlanid,        ParamDesc,  , %RegVlanid%
;HKR, Ndi\params\RegVlanid,        optional,   , "1"
HKR, Ndi\params\RegVlanid,        Type,       , "int"
HKR, Ndi\params\RegVlanid,        Default,    , "0"
HKR, Ndi\params\RegVlanid,        min,        , "0"
HKR, Ndi\params\RegVlanid,        max,        , "4094"
HKR, Ndi\params\RegVlanid,        step,       , "1"

;HKR,,PnPCapabilities,0x10001,0x0000

[PDPllDisabled.reg]
HKR,,PowerDownPll,0,"0"

[PDPllEnabled.reg]
HKR,,PowerDownPll,0,"1"

[DisablePBA.reg]
HKR,,DisablePBA,0,"1"

[EnablePBA.reg]
HKR,,DisablePBA,0,"0"

[AIPSModeEnable.reg]
HKR,,AIPSMode,0,"1"

[AIPSModeDisable.reg]
HKR,,AIPSMode,0,"0"

[ForceEnableClkReq.reg]
HKR,,ForceEnableClkReq,0,"1"

[GPPSWEnabled.reg]
HKR,,GPPSW,0,"1"

[DrvOption.reg]
HKR,Parameters,DrvOption,0x00010001,0

[DrvMode.reg]
HKR,Parameters,DrvMode,0x00010001,0

[SSEnabled.reg]
HKR,Parameters,SSEnabled,0x00010001,1

[CSEnabled.reg]
HKR,Parameters,CSEnabled,0x00010001,1

[DMAr.reg]
HKR,Parameters,DmaRemappingCompatible,0x00010001,2
;1 = opt-in, 2 = opt-in only for external devices

[S0MgcPktEnabled.reg]
HKR,,S0MgcPkt,0,"1"

[FiberMode1.reg]
HKR,,HwFiberModeVer,0x00010001,1
HKR,,HwFiberStat,0,"0"

[TRxOptThrld500.reg]
HKR,,TxOptimizeThreshold,0x00010001,0x1F4
HKR,,RxOptimizeThreshold,0x00010001,0x1F4

[TRxOptThrld1k.reg]
HKR,,TxOptimizeThreshold,0x00010001,0x3E8
HKR,,RxOptimizeThreshold,0x00010001,0x3E8

[DisableClkreqL1sub.reg]
HKR,,HwOption,0x00010001,0xD00000
HKR,,HwOptionV2,0x00010001,4

[DisableClkreqAndForceClkreq.reg]
HKR,,HwOption,0x00010001,0xC00000

[DisableForceClkreq.reg]
HKR,,HwOption,0x00010001,0x800000

[DisableIdleSpeedDown.reg]
HKR,,HwOptionV3,0x00010001,0x00040000


[del.reg]
HKR,Ndi\params

HKR,,*RscIPv4
HKR,,*RscIPv6
HKR,,ForceMode
HKR,,DisablePBA
HKR,,PowerDownPll
HKR,,ForceEnableClkReq
HKR,,JumboFrame
HKR,,AIPSMode
HKR,,S3S4WolPowerSaving
HKR,,LimitCbJumboFrame
HKR,,DeviceRemovable
HKR,,HwParaMask
HKR,,HwPciOtherFunDevMask
HKR,,HwOptimize
HKR,,HwOption
HKR,,HwWolCrcVal
HKR,,LogDisconnectEvent
HKR,,EnableEDT
HKR,,RIACP
HKR,,S5NicKeepOverrideMacAddr
HKR,,S5NicKeepOverrideMacAddrV2
HKR,,PPSW
HKR,,GPPSW
HKR,,S0MgcPkt
HKR,,HwFPSM
HKR,,SwIML
HKR,,SwIML100
HKR,,SwIMLV2
HKR,,SwIML100V2
HKR,,ENPWMode
HKR,,Diskless
HKR,,DisklessOption
HKR,,TxOptimizeThreshold
HKR,,RxOptimizeThreshold
HKR,,CFHTime
HKR,,LDWTime
HKR,,RMPT
HKR,,CRSPDThreshold
HKR,,ComboPerfAdjust
HKR,,CHNLWTime
HKR,,CHNLWCnt
HKR,,L1L0sLT
HKR,,MRRSize
HKR,,TDBSize
HKR,,RDBSize
HKR,,HwOptionV2
HKR,,HwOptionV3
HKR,,HwOptionV4
HKR,,HwBpMask
HKR,,MonitorModeEnabled
HKR,,UCEM
HKR,,HwFiberModeVer
HKR,,HwFiberStat
HKR,,FactoryMode
HKR,,RegVlanid
HKR,,AutoCrossoverDet
HKR,,S5WakeOnLan
HKR,,S5ARPOffload
HKR,,WolShutdownLinkSpeed
HKR,,AutoDisableGigabit
HKR,,AutoLinkDownPcieMacOff
HKR,,EnableGreenEthernet
HKR,,AdvancedEEE
HKR,,GigaLite
HKR,,WakeOnLinkUp
HKR,,WolCap
HKR,,PowerSavingMode
HKR,,EEEMaxSupportSpeed

[del.default.reg]
HKR,,*SpeedDuplex
HKR,,NetworkAddress
HKR,,*FlowControl
HKR,,*PriorityVLANTag
HKR,,*InterruptModeration
HKR,,*ReceiveBuffers
HKR,,*TransmitBuffers
HKR,,*JumboPacket
HKR,,*TCPChecksumOffloadIPv4
HKR,,*TCPChecksumOffloadIPv6
HKR,,*UDPChecksumOffloadIPv4
HKR,,*UDPChecksumOffloadIPv6
HKR,,*IPChecksumOffloadIPv4
HKR,,*LsoV1IPv4
HKR,,*LsoV2IPv4
HKR,,*LsoV2IPv6
HKR,,*RSS
HKR,,*NumRssQueues
HKR,,*WakeOnPattern
HKR,,*WakeOnMagicPacket
HKR,,*PMARPOffload
HKR,,*PMNSOffload
HKR,,*SelectiveSuspend
HKR,,*SSIdleTimeout
HKR,,*EEE
HKR,,EEE
HKR,,*HeaderDataSplit
HKR,,*IPSecOffloadV2
HKR,,*ModernStandbyWoLMagicPacket


;-----------------------------------------------------------------------------
; rtk NT specific
;

[rtk.reg]
HKR, Ndi,                       Service,    0, "e2kw10x64"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"


[rt640.Service]
DisplayName     = %rt640.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e2kw10x64.sys
LoadOrderGroup  = NDIS
AddReg          = DrvOption.reg, DrvMode.reg, DMAr.reg

[rt640SS.Service]
DisplayName     = %rt640.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e2kw10x64.sys
LoadOrderGroup  = NDIS
AddReg          = DrvOption.reg, DrvMode.reg, DMAr.reg
AddReg          = SSEnabled.reg

[rt640CS.Service]
DisplayName     = %rt640.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\e2kw10x64.sys
LoadOrderGroup  = NDIS
AddReg          = DrvOption.reg, DrvMode.reg, DMAr.reg
AddReg          = CSEnabled.reg


[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\e2kw10x64.sys"
HKR, , TypesSupported,   0x00010001, 7

;-----------------------------------------------------------------------------
; DestinationDirs
;
[rt640.CopyFiles]
e2kw10x64.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%


[SourceDisksFiles]
e2kw10x64.sys = 1,, ; on distribution disk 1


[DestinationDirs]
rt640.CopyFiles  = 12
DefaultDestDir     = 11

[Strings]
Killer                  = "Killer"
AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Speed & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Network Address"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
TxEnabled                = "Tx Enabled"
RxEnabled                = "Rx Enabled"
RxTxEnabled              = "Rx & Tx Enabled"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Flow Control"
PriorityVLAN             = "Priority & VLAN"
PriorityVLANDisabled     = "Priority & VLAN Disabled"
PriorityVLANEnabled      = "Priority & VLAN Enabled"
InterruptModeration      = "Interrupt Moderation"
ReceiveBuffers           = "Receive Buffers"
TransmitBuffers          = "Transmit Buffers"
AutoDisableGigabit       = "Auto Disable Gigabit"
AutoLinkDownPhyOff       = "Auto Disable PHY"
BatteryRe-Link           = "Re-Link, Battery"
AcBatteryRe-Link         = "Re-Link, Battery or AC"
Battery                  = "Enabled, Battery"
AcBattery                = "Enabled, Battery or AC"
JumboFrame               = "Jumbo Frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Auto Disable PCIe"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Auto Crossover Detection"
PriorityEnabled          = "Priority Enabled"
VLANEnabled              = "VLAN Enabled"
10MbFirst                = "10 Mbps First"
100MbFirst               = "100 Mbps First"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy-Efficient Ethernet"
HDSplit                  = "Header Data Split"
WakeOnLinkUp             = "Wake On Link Up"
NumRssQueues             = "Maximum Number of RSS Queues"
1Queue                   = "1 Queue"
2Queue                   = "2 Queues"
4Queue                   = "4 Queues"
IPSecv2                  = "IPsec Offload"
AH                       = "Auth Header Enabled"
ESP                      = "ESP Enabled"
AHESP                    = "Auth Header & ESP Enabled"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Arabic_UAX
[Strings.3801]
Killer                  = "Killer"
AutoDetect               = "التفاوض التلقائي"
SpeedDuplex              = "السرعة والازدواج"
10Mb-Half-Duplex         = "نصف المزدوج 10 ميجا بايت في الثانية"
10Mb-Full-Duplex         = "كامل الازدواج 10 ميجا بايت في الثانية"
100Mb-Half-Duplex        = "كامل الازدواج 100 ميجا بايت في الثانية"
100Mb-Full-Duplex        = "كامل الازدواج 100 ميجا بايت في الثانية"
1000Mb-Full-Duplex       = "كامل الازدواج 1000 ميجا بايت في الثانية"
2.5Gb-Full-Duplex        = "كامل الازدواج 2500 ميجا بايت في الثانية"
NetworkAddress           = "عنوان الشبكة"
IPChksumOffv4            = "تحميل المجموع الاختباري IPv4"
TCPChksumOffv4           = "تحميل المجموع الاختباري IPv4) TCP)"
UDPChksumOffv4           = "تحميل المجموع الاختباري IPv4) UDP)"
TCPChksumOffv6           = "تحميل المجموع الاختباري IPv6) TCP)"
UDPChksumOffv6           = "تحميل المجموع الاختباري IPv6) UDP)"
Enabled                  = "قيد التمكين"
Disabled                 = "قيد التعطيل"
TxEnabled                = "Tx قيد التمكين"
RxEnabled                = "Rx قيد التمكين"
RxTxEnabled              = "Rx & Tx قيد التمكين"
LSOv4                    = "تحميل الإرسال الكبير (IPv4)"
LSOv2v4                  = "تحميل الإرسال الكبير IPv4) v2)"
LSOv2v6                  = "تحميل الإرسال الكبير IPv6) v2)"
FlowControl              = "التحكم بالانسياب"
PriorityVLAN             = "الأولوية وVLAN"
PriorityVLANDisabled     = "الأولوية وVLAN قيد التعطيل"
PriorityVLANEnabled      = "الأولوية وVLAN قيد التمكين"
InterruptModeration      = "قطع التوسط"
ReceiveBuffers           = "استقبال المخزنات المؤقتة"
TransmitBuffers          = "نقل المخزنات المؤقتة"
AutoDisableGigabit       = "تعطيل تلقائي جيجا بت (PowerSaving)"
AutoLinkDownPhyOff       = "تعطيل تلقائي PowerSaving) PHY)"
BatteryRe-Link           = "إعادة الربط، البطارية"
AcBatteryRe-Link         = "إعادة الربط، البطارية أو التيار المتردد"
Battery                  = "قيد التمكين، البطارية"
AcBattery                = "قيد التمكين، البطارية أو التيار المتردد"
JumboFrame               = "الإطار الضخم"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "إغلاق معيار Wake-On-Lan"
AutoLinkDownPcieMacOff   = "تعطيل تلقائي PowerSaving) PCIe)"
RSS                      = "استلام تحديد مقياس الجانب"
AutoCrossoverDet         = "رصد التحويل التلقائي"
PriorityEnabled          = "الأولوية قيد التمكين"
VLANEnabled              = "VLAN قيد التمكين"
10MbFirst                = "10 ميجا بايت في الثانية أولا"
100MbFirst               = "100 ميجا بايت في الثانية أولا"
WolShutdownLinkSpeed     = "رابط السرعة للإغلاق وWOL"
NotSpeedDown             = "عدم تخفيض السرعة"
WolCap                   = "قدرات تنشيط Lan"
None                     = "لا شيء"
PatternMatch             = "مطابقة عامل البحث"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "مطابقة عامل البحث وMagic Packet"
GreenEthernet            = "إيثرنت أخضر"
WakeOnPtn                = "التنبيه عند مطابقة النقش"
WakeOnMagPkt             = "لتنبيه عند الحزمة السحرية"
ARPOffload               = "ARP توزيع نقل بيانات "
NsOffload                = " توزيع نقل بيانات NS"
EEE                      = " تقنية إيثرنت لحفظ الطاقة "
HDSplit                  = "نقسام بيانات الرأس"
WakeOnLinkUp             = "لتنبيه عند الارتباط"
NumRssQueues             = "RSS لعدد الأقصى لقوائم انتظار "
1Queue                   = "قائمة انتظار واحدة"
2Queue                   = "قائمتا انتظار"
4Queue                   = " 4 قوائم انتظار"
IPSecv2                  = "IPsec توزيع نقل بيانات "
AH                       = "تم تمكين رأس المصادقة"
ESP                      = "ESP تم تمكين "
AHESP                    = "ESP تم تمكين رأس المصادقة و"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Bulgarian
[Strings.0402]
Killer                  = "Killer"
AutoDetect               = "Автоматични преговори"
SpeedDuplex              = "Скорост и дуплекс"
10Mb-Half-Duplex         = "10 Mbps полудуплекс"
10Mb-Full-Duplex         = "10 Mbps пълен дуплекс"
100Mb-Half-Duplex        = "100 Mbps полудуплекс"
100Mb-Full-Duplex        = "100 Mbps пълен дуплекс"
1000Mb-Full-Duplex       = "1,0 Gbps пълен дуплекс"
2.5Gb-Full-Duplex        = "2,5 Gbps пълен дуплекс"
NetworkAddress           = "Мрежов адрес"
IPChksumOffv4            = "Контролна сума IPv4 при разтоварване"
TCPChksumOffv4           = "Контролна сума TCP при разтоварване (IPv4)"
UDPChksumOffv4           = "Контролна сума UDP при разтоварване (IPv4)"
TCPChksumOffv6           = "Контролна сума TCP при разтоварване (IPv6)"
UDPChksumOffv6           = "Контролна сума UDP при разтоварване (IPv6)"
Enabled                  = "Разрешено"
Disabled                 = "Забранено"
TxEnabled                = "Tx разрешен"
RxEnabled                = "Rx разрешен"
RxTxEnabled              = "Rx & Tx Разрешено"
LSOv4                    = "Голямо разтоварване на изпращане (IPv4)"
LSOv2v4                  = "Голямо разтоварване на изпращане в2 (IPv4)"
LSOv2v6                  = "Голямо разтоварване на изпращане в2 (IPv6)"
FlowControl              = "Управление на потока"
PriorityVLAN             = "Приоритет и VLAN"
PriorityVLANDisabled     = "Приоритет и VLAN забранени"
PriorityVLANEnabled      = "Приоритет и VLAN разрешени"
InterruptModeration      = "Прекъсване на наблюдаване"
ReceiveBuffers           = "Буфери при получаване"
TransmitBuffers          = "Буфери при прехвърляне"
AutoDisableGigabit       = "Автоматично забрани Gigabit (Икономия на енергия)"
AutoLinkDownPhyOff       = "Автоматично забрани PHY (Икономия на енергия)"
BatteryRe-Link           = "Повторна връзка, батерия"
AcBatteryRe-Link         = "Повторна връзка, батерия или променлив ток"
Battery                  = "Разрешено, батерия"
AcBattery                = "Разрешено, батерия или променлив ток"
JumboFrame               = "Jumbo рамка"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Изключване на събуждане при LAN"
AutoLinkDownPcieMacOff   = "Автоматично забрани PCIe (Икономия на енергия)"
RSS                      = "Получаване на мащабиране на страните"
AutoCrossoverDet         = "Авт. откриване на кросовър"
PriorityEnabled          = "Разрешен приоритет"
VLANEnabled              = "VLAN разрешена"
10MbFirst                = "10 Mbps първо"
100MbFirst               = "100 Mbps първо"
WolShutdownLinkSpeed     = "WOL & скорост на връзката при изключване"
NotSpeedDown             = "Няма намаляване на скоростта"
WolCap                   = "Събуждане при LAN "
None                     = "Няма"
PatternMatch             = "Съвпадение на модел"
MagicPacket              = "Магически пакет"
PatternAndMagic          = "Съвпадение на модел и магически пакет"
GreenEthernet            = "Зелена Ethernet мрежа"
WakeOnPtn                = "Събуждане при съвпадение на модел"
WakeOnMagPkt             = "Събуждане при Magic Packet"
ARPOffload               = "ARP офлоуд"
NsOffload                = "NS офлоуд"
EEE                      = "Енергийно ефективен Етернет"
HDSplit                  = "Разделяне на Заглавните данни"
WakeOnLinkUp             = "Събуждане при Линк"
NumRssQueues             = "Максимален брой на RSS редица"
1Queue                   = "1 редица"
2Queue                   = "2 редици"
4Queue                   = "4 редици"
IPSecv2                  = "IPsec офлоуд"
AH                       = "Заглавен сертификат е активиран"
ESP                      = "ESP е активиран"
AHESP                    = "Заглавен сертификат & ESP са активирани"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Chinese_Taiwan
[Strings.0404]
Killer                  = "Killer"
AutoDetect               = "自動偵測"
SpeedDuplex              = "連線速度與雙工模式"
10Mb-Half-Duplex         = "10 Mbps 半雙工"
10Mb-Full-Duplex         = "10 Mbps 全雙工"
100Mb-Half-Duplex        = "100 Mbps 半雙工"
100Mb-Full-Duplex        = "100 Mbps 全雙工"
1000Mb-Full-Duplex       = "1.0 Gbps 全雙工"
2.5Gb-Full-Duplex        = "2.5 Gbps 全雙工"
NetworkAddress           = "網路卡位址"
IPChksumOffv4            = "IPv4 檢查總和值卸載"
TCPChksumOffv4           = "TCP 檢查總和卸載 (IPv4)"
UDPChksumOffv4           = "UDP 檢查總和卸載 (IPv4)"
TCPChksumOffv6           = "TCP 檢查總和卸載 (IPv6)"
UDPChksumOffv6           = "UDP 檢查總和卸載 (IPv6)"
Enabled                  = "開啟"
Disabled                 = "關閉"
TxEnabled                = "Tx 開啟"
RxEnabled                = "Rx 開啟"
RxTxEnabled              = "Rx & Tx 開啟"
LSOv4                    = "大量傳送卸載 (IPv4)"
LSOv2v4                  = "大量傳送卸載 v2 (IPv4)"
LSOv2v6                  = "大量傳送卸載 v2 (IPv6)"
FlowControl              = "流量控制"
PriorityVLAN             = "優先權 & VLAN"
PriorityVLANDisabled     = "優先權 & VLAN 關閉"
PriorityVLANEnabled      = "優先權 & VLAN 開啟"
InterruptModeration      = "中斷調整合適化"
ReceiveBuffers           = "接收緩衝區"
TransmitBuffers          = "傳送緩衝區"
AutoDisableGigabit       = "自動關閉 Gigabit"
AutoLinkDownPhyOff       = "自動關閉 PHY"
BatteryRe-Link           = "重新連線, 電池"
AcBatteryRe-Link         = "重新連線, 電池或 AC"
Battery                  = "開啟, 電池"
AcBattery                = "開啟, 電池或 AC"
JumboFrame               = "巨大訊框"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "關機網路喚醒"
AutoLinkDownPcieMacOff   = "自動關閉 PCIe"
RSS                      = "接收端調整"
AutoCrossoverDet         = "自動跳線偵測"
PriorityEnabled          = "優先權開啟"
VLANEnabled              = "VLAN 開啟"
10MbFirst                = "10 Mbps 優先"
100MbFirst               = "100 Mbps 優先"
WolShutdownLinkSpeed     = "WOL & 關機連線速度"
NotSpeedDown             = "不降速"
WolCap                   = "網路喚醒能力"
None                     = "無"
PatternMatch             = "樣式比對"
MagicPacket              = "魔術封包"
PatternAndMagic          = "樣式比對及魔術封包"
GreenEthernet            = "環保節能"
WakeOnPtn                = "樣式比對喚醒"
WakeOnMagPkt             = "魔術封包喚醒"
ARPOffload               = "ARP 卸載"
NsOffload                = "NS 卸載"
EEE                      = "節能乙太網路"
HDSplit                  = "表頭資料切割"
WakeOnLinkUp             = "連線喚醒"
NumRssQueues             = "接收端調整最大佇列"
1Queue                   = "1個佇列"
2Queue                   = "2個佇列"
4Queue                   = "4個佇列"
IPSecv2                  = "IPsec 卸載"
AH                       = "Auth 表頭開啟"
ESP                      = "ESP 開啟"
AHESP                    = "Auth 表頭 & ESP 開啟"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Chinese (PRC)
[Strings.0804]
Killer                  = "Killer"
AutoDetect               = "自动侦测"
SpeedDuplex              = "连接速度和双工模式"
10Mb-Half-Duplex         = "10 Mbps 半双工"
10Mb-Full-Duplex         = "10 Mbps 全双工"
100Mb-Half-Duplex        = "100 Mbps 半双工"
100Mb-Full-Duplex        = "100 Mbps 全双工"
1000Mb-Full-Duplex       = "1.0 Gbps 全双工"
2.5Gb-Full-Duplex        = "2.5 Gbps 全双工"
NetworkAddress           = "网络地址"
IPChksumOffv4            = "IPv4 硬件校验和"
TCPChksumOffv4           = "TCP 硬件校验和 (IPv4)"
UDPChksumOffv4           = "UDP 硬件校验和 (IPv4)"
TCPChksumOffv6           = "TCP 硬件校验和 (IPv6)"
UDPChksumOffv6           = "UDP 硬件校验和 (IPv6)"
Enabled                  = "开启"
Disabled                 = "关闭"
TxEnabled                = "Tx 开启"
RxEnabled                = "Rx 开启"
RxTxEnabled              = "Rx & Tx 开启"
LSOv4                    = "大量传送减负 (IPv4)"
LSOv2v4                  = "大量传送减负 v2 (IPv4)"
LSOv2v6                  = "大量传送减负 v2 (IPv6)"
FlowControl              = "流控制"
PriorityVLAN             = "优先级和VLAN"
PriorityVLANDisabled     = "优先级和VLAN 关闭"
PriorityVLANEnabled      = "优先级和VLAN 开启"
InterruptModeration      = "中断调整"
ReceiveBuffers           = "接收缓冲区"
TransmitBuffers          = "传送缓冲区"
AutoDisableGigabit       = "自动关闭 Gigabit"
AutoLinkDownPhyOff       = "自动关闭 PHY"
BatteryRe-Link           = "重新联接, 电池"
AcBatteryRe-Link         = "重新联接, 电池或者交流电源"
Battery                  = "开启, 电池"
AcBattery                = "开启, 电池或者交流电源"
JumboFrame               = "巨型帧"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "关机 网络唤醒"
AutoLinkDownPcieMacOff   = "自动关闭 PCIe"
RSS                      = "接收端调整"
AutoCrossoverDet         = "自动跳线侦测"
PriorityEnabled          = "优先级开启"
VLANEnabled              = "VLAN 开启"
10MbFirst                = "10 Mbps 优先"
100MbFirst               = "100 Mbps 优先"
WolShutdownLinkSpeed     = "网络唤醒和关机连接速度"
NotSpeedDown             = "不降速"
WolCap                   = "网络唤醒能力"
None                     = "无"
PatternMatch             = "样式比对"
MagicPacket              = "魔术封包"
PatternAndMagic          = "样式比对及魔术封包"
GreenEthernet            = "环保节能"
WakeOnPtn                = "样式比对唤醒"
WakeOnMagPkt             = "魔术封包唤醒"
ARPOffload               = "ARP 减负"
NsOffload                = "NS 减负"
EEE                      = "节能乙太网路"
HDSplit                  = "表头资料切割"
WakeOnLinkUp             = "连线唤醒"
NumRssQueues             = "接收端调整最大伫列"
1Queue                   = "1个伫列"
2Queue                   = "2个伫列"
4Queue                   = "4个伫列"
IPSecv2                  = "IPsec 减负"
AH                       = "Auth 表头开启"
ESP                      = "ESP 开启"
AHESP                    = "Auth 表头 & ESP 开启"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Croatian
[Strings.041a]
Killer                  = "Killer"
AutoDetect               = "Automatsko prilagođivanje"
SpeedDuplex              = "Brzina i dupleks"
10Mb-Half-Duplex         = "10 Mb/s poludupleks"
10Mb-Full-Duplex         = "10 Mb/s puni dupleks"
100Mb-Half-Duplex        = "100 Mb/s poludupleks"
100Mb-Full-Duplex        = "100 Mb/s puni dupleks"
1000Mb-Full-Duplex       = "1.0 Gb/s puni dupleks"
2.5Gb-Full-Duplex        = "2.5 Gb/s puni dupleks"
NetworkAddress           = "Mrežna adresa"
IPChksumOffv4            = "IPv4 kontrolni zbroj bez opterećenja"
TCPChksumOffv4           = "TCP kontrolni zbroj na periferiju (IPv4)"
UDPChksumOffv4           = "UDP kontrolni zbroj na periferiju (IPv4)"
TCPChksumOffv6           = "TCP kontrolni zbroj na periferiju (IPv6)"
UDPChksumOffv6           = "UDP kontrolni zbroj na periferiju (IPv6)"
Enabled                  = "Omogućeno"
Disabled                 = "Onemogućeno"
TxEnabled                = "Tx omogućeno"
RxEnabled                = "Rx omogućeno"
RxTxEnabled              = "Rx & Tx omogućeno"
LSOv4                    = "Slanje velikog na periferiju (IPv4)"
LSOv2v4                  = "Slanje velikog na periferiju v2 (IPv4)"
LSOv2v6                  = "Slanje velikog na periferiju v2 (IPv6)"
FlowControl              = "Kontrola protoka"
PriorityVLAN             = "Prioritet i VLAN"
PriorityVLANDisabled     = "Prioritet i VLAN onemogućen"
PriorityVLANEnabled      = "Prioritet i VLAN omogućeni"
InterruptModeration      = "Moderacija prekida"
ReceiveBuffers           = "Spremnici prijema"
TransmitBuffers          = "Spremnici prijenosa"
AutoDisableGigabit       = "Automatsko isključivanje Gigabita"
AutoLinkDownPhyOff       = "Automatsko isključivanje PHY"
BatteryRe-Link           = "Re-Link, baterija"
AcBatteryRe-Link         = "Re-Link, baterija ili AC napajanje"
Battery                  = "Omogućeno, baterija"
AcBattery                = "Omogućeno, baterije ili AC"
JumboFrame               = "Jumbo okvir"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Isključivanje funkcije Probudi se na mreži nakon isključivanja"
AutoLinkDownPcieMacOff   = "Automatsko isključivanje PCIe"
RSS                      = "Smanjivanje na strani prijema"
AutoCrossoverDet         = "Automatska detekcija preslušavanja"
PriorityEnabled          = "Prioritet omogućen"
VLANEnabled              = "VLAN omogućen"
10MbFirst                = "Prvo 10 Mb/s"
100MbFirst               = "Prvo 100 Mb/s"
WolShutdownLinkSpeed     = "Brzina veze za WOL i isključivanje"
NotSpeedDown             = "Nema smanjivanja brzine"
WolCap                   = "Mogućnosti Probudi se na mreži"
None                     = "Nema"
PatternMatch             = "Podudarnost obrasca"
MagicPacket              = "Magični paket"
PatternAndMagic          = "Podudarnost obrasca i magični paket"
GreenEthernet            = "Zeleni Ethernet"
WakeOnPtn                = "Odgovarajući uzorak izlaska iz stanja mirovanja"
WakeOnMagPkt             = "Čarobni paket izlaska iz stanja mirovanja"
ARPOffload               = "ARP rasterećenje"
NsOffload                = "NS rasterećenje"
EEE                      = "Energetski učinkovit Ethernet"
HDSplit                  = "Razdijeljeni podaci zaglavlja"
WakeOnLinkUp             = "Povezivanje pri izlasku iz stanja mirovanja"
NumRssQueues             = "Maksimalni broj RSS redova čekanja"
1Queue                   = "1 red čekanja"
2Queue                   = "2 reda čekanja"
4Queue                   = "4 reda čekanja"
IPSecv2                  = "IPsec rasterećenje"
AH                       = "Zaglavlje provjere autentičnosti omogućeno"
ESP                      = "ESP omogućeno"
AHESP                    = "Zaglavlje provjere autentičnosti i ESP omogućeni"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; CZ
[Strings.0405]
Killer                  = "Killer"
AutoDetect               = "Automatické nastavení režimu provozu"
SpeedDuplex              = "Rychlost a přenosový režim"
10Mb-Half-Duplex         = "Poloduplexní 10 Mbps"
10Mb-Full-Duplex         = "Plně duplexní 10 Mbps"
100Mb-Half-Duplex        = "Poloduplexní 100 Mbps"
100Mb-Full-Duplex        = "Plně duplexní 100 Mbps"
1000Mb-Full-Duplex       = "Plně duplexní 1,0 Gbps"
2.5Gb-Full-Duplex        = "Plně duplexní 2,5 Gbps"
NetworkAddress           = "Síťová adresa"
IPChksumOffv4            = "Výpočet kontrolních součtů protokolu IPv4"
TCPChksumOffv4           = "Výpočet kontrolních součtů protokolu TCP (IPv4)"
UDPChksumOffv4           = "Výpočet kontrolních součtů protokolu UDP (IPv4)"
TCPChksumOffv6           = "Výpočet kontrolních součtů protokolu TCP (IPv6)"
UDPChksumOffv6           = "Výpočet kontrolních součtů protokolu UDP (IPv6)"
Enabled                  = "Povoleno"
Disabled                 = "Zakázáno"
TxEnabled                = "Odesílání povoleno"
RxEnabled                = "Příjem povolen"
RxTxEnabled              = "Příjem a odesílání povoleno"
LSOv4                    = "Zpracování velkých segmentů LSO (IPv4)"
LSOv2v4                  = "Zpracování velkých segmentů LSO v2 (IPv4)"
LSOv2v6                  = "Zpracování velkých segmentů LSO v2 (IPv6)"
FlowControl              = "Řízení toku"
PriorityVLAN             = "Priorita a VLAN"
PriorityVLANDisabled     = "Priorita a VLAN zakázána"
PriorityVLANEnabled      = "Priorita a VLAN povolena"
InterruptModeration      = "Tlumení přerušení"
ReceiveBuffers           = "Zásobníky příjmu"
TransmitBuffers          = "Zásobníky odesílání"
AutoDisableGigabit       = "Automatická deaktivace gigabitové sítě"
AutoLinkDownPhyOff       = "Automatická deaktivace PHY"
BatteryRe-Link           = "Re-link, baterie"
AcBatteryRe-Link         = "Re-link, baterie nebo AC"
Battery                  = "Povoleno, baterie"
AcBattery                = "Povoleno, baterie nebo AC"
JumboFrame               = "Jumbo rámec"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Automatická deaktivace PCIe"
RSS                      = "Škálování na straně příjmu"
AutoCrossoverDet         = "Automatická detekce křížených kabelů"
PriorityEnabled          = "Priorita povolena"
VLANEnabled              = "VLAN povolena"
10MbFirst                = "Nejdříve 10 Mbps"
100MbFirst               = "Nejdříve 100 Mbps"
WolShutdownLinkSpeed     = "Rychlost linky pro WOL a vypnutí"
NotSpeedDown             = "Bez zpomalení"
WolCap                   = "Možnosti zapnutí počítače přes síť"
None                     = "Žádný"
PatternMatch             = "Shoda řetězce"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Shoda řetězce a Magic Packet"
GreenEthernet            = "Zelený Ethernet"
WakeOnPtn                = "Probuzení porovnávacím vzorkem"
WakeOnMagPkt             = "Probuzení paketem Magic"
ARPOffload               = "Snižování zatížení ARP"
NsOffload                = "Snižování zatížení NS"
EEE                      = "Úsporná síť Ethernet"
HDSplit                  = "Rozdělení dat hlavičky"
WakeOnLinkUp             = "Přenos probuzením"
NumRssQueues             = "Maximální počet front RSS"
1Queue                   = "1 fronta"
2Queue                   = "2 fronty"
4Queue                   = "4 fronty"
IPSecv2                  = "Snižování zatížení IPsec"
AH                       = "Protokol AH povolen"
ESP                      = "Protokol ESP povolen"
AHESP                    = "Protokoly AH a ESP byly povoleny"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Danish
[Strings.0406]
Killer                  = "Killer"
AutoDetect               = "Automatisk forhandling"
SpeedDuplex              = "Hastighed og duplex"
10Mb-Half-Duplex         = "10 Mbps halv duplex"
10Mb-Full-Duplex         = "10 Mbps fuld duplex"
100Mb-Half-Duplex        = "100 Mbps halv duplex"
100Mb-Full-Duplex        = "100 Mbps fuld duplex"
1000Mb-Full-Duplex       = "1.0 Gbps fuld duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps fuld duplex"
NetworkAddress           = "Netværksadresse"
IPChksumOffv4            = "Aflastning af IPv4 kontrolsum"
TCPChksumOffv4           = "Aflastning af TCP kontrolsum (IPv4)"
UDPChksumOffv4           = "Aflastning af UDP kontrolsum (IPv4)"
TCPChksumOffv6           = "Aflastning af TCP kontrolsum (IPv6)"
UDPChksumOffv6           = "Aflastning af UDP kontrolsum (IPv6)"
Enabled                  = "Aktiveret"
Disabled                 = "Deaktiveret"
TxEnabled                = "Tx aktiveret"
RxEnabled                = "Rx aktiveret"
RxTxEnabled              = "Rx og Tx aktiveret"
LSOv4                    = "Aflastning af stor forsendelse (IPv4)"
LSOv2v4                  = "Aflastning af stor forsendelse v2 (IPv4)"
LSOv2v6                  = "Aflastning af stor forsendelse v2 (IPv6)"
FlowControl              = "Flow-kontrol"
PriorityVLAN             = "Prioritet og VLAN"
PriorityVLANDisabled     = "Prioritet og VLAN deaktiveret"
PriorityVLANEnabled      = "Prioritet og VLAN aktiveret"
InterruptModeration      = "Interruptindstilling"
ReceiveBuffers           = "Modtagelsesbuffer"
TransmitBuffers          = "Afsendelsesbuffere"
AutoDisableGigabit       = "Automatisk deaktivering af gigabit"
AutoLinkDownPhyOff       = "Automatisk deaktivering af PHY"
BatteryRe-Link           = "Genetabler forbindelse, batteri"
AcBatteryRe-Link         = "Genetabler forbindelse, batteri eller AC"
Battery                  = "Aktiveret, batteri"
AcBattery                = "Aktiveret, batteri eller AC"
JumboFrame               = "Jumboramme"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Nedluk Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Automatisk deaktivering af PCIe"
RSS                      = "Skalering, modtagelsesside"
AutoCrossoverDet         = "Detektering af automatisk crossover"
PriorityEnabled          = "Prioritet aktiveret"
VLANEnabled              = "VLAN aktiveret"
10MbFirst                = "10 Mbps først"
100MbFirst               = "100 Mbps først"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Grøn Ethernet"
WakeOnPtn                = "Vågn op ved mønstergenkendelse"
WakeOnMagPkt             = "Vågn op ved Magisk pakke"
ARPOffload               = "ARP-aflastning"
NsOffload                = "NS-aflastning"
EEE                      = "Energibesparende Ethernet"
HDSplit                  = "Opdel headerdata"
WakeOnLinkUp             = "Vågn op ved sammenkædning"
NumRssQueues             = "Maksimal antal RSS-køer"
1Queue                   = "1 kø"
2Queue                   = "2 køer"
4Queue                   = "4 køer"
IPSecv2                  = "IPsec-aflastning"
AH                       = "Godkendelsesheader er aktiveret"
ESP                      = "ESP er aktiveret"
AHESP                    = "Godkendelsesheader & ESP er aktiveret"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Dutch
[Strings.0413]
Killer                  = "Killer"
AutoDetect               = "Automatisch onderhandelen"
SpeedDuplex              = "Snelheid & duplex"
10Mb-Half-Duplex         = "10 Mbps Half duplex"
10Mb-Full-Duplex         = "10 Mbps Full duplex"
100Mb-Half-Duplex        = "100 Mbps Half duplex"
100Mb-Full-Duplex        = "100 Mbps Full duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Netwerkadres"
IPChksumOffv4            = "IPv4-checksum-offload"
TCPChksumOffv4           = "TCP-checksum-offload (IPv4)"
UDPChksumOffv4           = "UDP-checksum-offload (IPv4)"
TCPChksumOffv6           = "TCP-checksum-offload (IPv6)"
UDPChksumOffv6           = "UDP-checksum-offload (IPv6)"
Enabled                  = "Ingeschakeld"
Disabled                 = "Uitgeschakeld"
TxEnabled                = "Tx ingeschakeld"
RxEnabled                = "Rx ingeschakeld"
RxTxEnabled              = "Rx & Tx ingeschakeld"
LSOv4                    = "Grote verzendings-offload (IPv4)"
LSOv2v4                  = "Grote verzendings-Offload v2 (IPv4)"
LSOv2v6                  = "Grote verzendings-Offload v2 (IPv6)"
FlowControl              = "Datatransportbesturing"
PriorityVLAN             = "Prioriteit & VLAN"
PriorityVLANDisabled     = "Prioriteit & VLAN uitgeschakeld"
PriorityVLANEnabled      = "Prioriteit & VLAN ingeschakeld"
InterruptModeration      = "Interrupt-controle"
ReceiveBuffers           = "Buffers ontvangst"
TransmitBuffers          = "Buffers verzending"
AutoDisableGigabit       = "Gigabit automatisch uitschakelen"
AutoLinkDownPhyOff       = "PHY automatisch uitschakelen"
BatteryRe-Link           = "Opnieuw verbinden, batterij"
AcBatteryRe-Link         = "Opnieuw verbinden, batterij of AC"
Battery                  = "Ingeschakeld, batterij"
AcBattery                = "Ingeschakeld, batterij of AC"
JumboFrame               = "Jumbo frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Wake-On-LAN uitschakelen"
AutoLinkDownPcieMacOff   = "PCIe automatisch uitschakelen"
RSS                      = "Schaling ontvangstzijde"
AutoCrossoverDet         = "Automatische kruislingse detectie"
PriorityEnabled          = "Prioriteit ingeschakeld"
VLANEnabled              = "VLAN ingeschakeld"
10MbFirst                = "10 Mbps eerst"
100MbFirst               = "100 Mbps eerst"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Patroonovereenkomst"
MagicPacket              = "Magisch pakket"
PatternAndMagic          = "Patroonovereenkomst & Magisch pakket"
GreenEthernet            = "Groen Ethernet"
WakeOnPtn                = "Ontwaken bij overeenkomend patroon"
WakeOnMagPkt             = "Ontwaken door Magic Packet"
ARPOffload               = "ARP-ontlading"
NsOffload                = "NS-ontlading"
EEE                      = "Energie-efficiënt Ethernet"
HDSplit                  = "Splitsen header-gegevens"
WakeOnLinkUp             = "Ontwaken door opkomen koppeling"
NumRssQueues             = "Maximaal aantal RSS-wachtrijen"
1Queue                   = "1 wachtrij"
2Queue                   = "2 wachtrijen"
4Queue                   = "4 wachtrijen"
IPSecv2                  = "IPSec-ontlading"
AH                       = "Ver. header ingeschakeld"
ESP                      = "ESP ingeschakeld"
AHESP                    = "Ver. header en ESP ingeschakeld"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Finnish
[Strings.040B]
Killer                  = "Killer"
AutoDetect               = "Automaattinen neuvottelu"
SpeedDuplex              = "Nopeus & Duplex"
10Mb-Half-Duplex         = "10 Mbps puolikas Duplex"
10Mb-Full-Duplex         = "10 Mbps täysi Duplex"
100Mb-Half-Duplex        = "100 Mbps puolikas Duplex"
100Mb-Full-Duplex        = "100 Mbps täysi Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps täysi Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps täysi Duplex"
NetworkAddress           = "Verkon osoite"
IPChksumOffv4            = "IPv4 Pura tarkistussumma"
TCPChksumOffv4           = "TCP Pura tarkistussumma (IPv4)"
UDPChksumOffv4           = "UDP Pura tarkistussumma (IPv4)"
TCPChksumOffv6           = "TCP Pura tarkistussumma (IPv6)"
UDPChksumOffv6           = "UDP Pura tarkistussumma (IPv6)"
Enabled                  = "Käytössä"
Disabled                 = "Poistettu käytöstä"
TxEnabled                = "Tx Käytössä"
RxEnabled                = "Rx Käytössä"
RxTxEnabled              = "Rx & Tx Käytössä"
LSOv4                    = "Pura isot lähetykset (IPv4)"
LSOv2v4                  = "Pura isot lähetykset v2 (IPv4)"
LSOv2v6                  = "Pura isot lähetykset v2 (IPv6)"
FlowControl              = "Datavuon ohjaus"
PriorityVLAN             = "Etusija & VLAN"
PriorityVLANDisabled     = "Etusija & VLAN poistettu käytöstä"
PriorityVLANEnabled      = "Etusija & VLAN käytössä"
InterruptModeration      = "Keskeytyksen hidastaminen"
ReceiveBuffers           = "Vastaanota puskureita"
TransmitBuffers          = "Siirrä puskureita"
AutoDisableGigabit       = "Ota Gigabit automaattisesti pois päältä"
AutoLinkDownPhyOff       = "Ota PHY automaattisesti pois päältä"
BatteryRe-Link           = "Linkitä uudelleen, akku"
AcBatteryRe-Link         = "Linkitä uudelleen, akku tai verkkovirta"
Battery                  = "Käytössä, akku"
AcBattery                = "Käytössä, akku tai verkkovirta"
JumboFrame               = "Jumbo Frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Sammuta herätystoiminto Lanin kautta"
AutoLinkDownPcieMacOff   = "Ota PCIe automaattisesti pois päältä"
RSS                      = "RSS-verkkosyötemuodot"
AutoCrossoverDet         = "Automaattinen ohitustunnistin"
PriorityEnabled          = "Etusija käytössä"
VLANEnabled              = "VLAN käytössä"
10MbFirst                = "10 Mbps ensin"
100MbFirst               = "100 Mbps ensin"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Vihreä Ethernet"
WakeOnPtn                = "Herätys vastaavalla kuviolla"
WakeOnMagPkt             = "Herätys Magic Packet -sovelluksella"
ARPOffload               = "ARP-purkaminen"
NsOffload                = "NS-purkaminen"
EEE                      = "Energiatehokas Ethernet"
HDSplit                  = "Otsikkotietojen lohkominen"
WakeOnLinkUp             = "Herätys Link Up -sovelluksella"
NumRssQueues             = "RSS-jonojen maksimimäärä"
1Queue                   = "1 jono"
2Queue                   = "2 jonoa"
4Queue                   = "4 jonoa"
IPSecv2                  = "Ipsec-purkaminen"
AH                       = "Valtuutusotsikko käytössä"
ESP                      = "ESP käytössä"
AHESP                    = "Valtuutusotsikko ja ESP käytössä"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; French
[Strings.040c]
Killer                  = "Killer"
AutoDetect               = "Négociation auto"
SpeedDuplex              = "Vitesse & Duplex"
10Mb-Half-Duplex         = "10 Mbps Semi-duplex"
10Mb-Full-Duplex         = "10 Mbps Duplex intégral"
100Mb-Half-Duplex        = "100 Mbps Semi-duplex"
100Mb-Full-Duplex        = "100 Mbps Duplex intégral"
1000Mb-Full-Duplex       = "1.0 Gbps Duplex intégral"
2.5Gb-Full-Duplex        = "2.5 Gbps Duplex intégral"
NetworkAddress           = "Adresse de réseau"
IPChksumOffv4            = "IPv4 Somme de contrôle hors charge"
TCPChksumOffv4           = "TCP Somme de contrôle hors charge (IPv4)"
UDPChksumOffv4           = "UDP Somme de contrôle hors charge (IPv4)"
TCPChksumOffv6           = "TCP Somme de contrôle hors charge (IPv6)"
UDPChksumOffv6           = "UDP Somme de contrôle hors charge (IPv6)"
Enabled                  = "Activé"
Disabled                 = "Désactivé"
TxEnabled                = "Tx activé"
RxEnabled                = "Rx activé"
RxTxEnabled              = "Rx & Tx activé"
LSOv4                    = "Grand envoi hors charge (IPv4)"
LSOv2v4                  = "Grand envoi hors charge v2 (IPv4)"
LSOv2v6                  = "Grand envoi hors charge v2 (IPv6)"
FlowControl              = "Contrôle de flux"
PriorityVLAN             = "Priorité & VLAN"
PriorityVLANDisabled     = "Priorité & VLAN désactivé"
PriorityVLANEnabled      = "Priorité & VLAN activé"
InterruptModeration      = "Modération interruption"
ReceiveBuffers           = "Mémoires tampon de réception"
TransmitBuffers          = "Mémoires tampon de transmission"
AutoDisableGigabit       = "Désactiver auto gigaoctet"
AutoLinkDownPhyOff       = "Désactiver auto PHY"
BatteryRe-Link           = "Re-lier, Batterie"
AcBatteryRe-Link         = "Re-lier, Batterie ou AC"
Battery                  = "Activé, Batterie"
AcBattery                = "Activé, Batterie ou AC"
JumboFrame               = "Cadre jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Arrêter Réveil par réseau"
AutoLinkDownPcieMacOff   = "Désactiver auto PCIe"
RSS                      = "Echelle coté réception"
AutoCrossoverDet         = "Détection auto inversion"
PriorityEnabled          = "Priorité activé"
VLANEnabled              = "VLAN activé"
10MbFirst                = "10 Mbps en premier"
100MbFirst               = "100 Mbps en premier"
WolShutdownLinkSpeed     = "WoL / Arrêt vitesse réseau"
NotSpeedDown             = "Pas vitesse ralentie"
WolCap                   = "Fonctions Réveil par le réseau"
None                     = "Aucun"
PatternMatch             = "Correspondance au modèle"
MagicPacket              = "Paquet Magic"
PatternAndMagic          = "Correspondance au modèle et Paquet Magic"
GreenEthernet            = "Ethernet vert"
WakeOnPtn                = "Avertir lors de correspondance de motif"
WakeOnMagPkt             = "Réveil sur Magic Packet"
ARPOffload               = "Décharge ARP"
NsOffload                = "Décharge NS"
EEE                      = "Ethernet à économie d’énergie"
HDSplit                  = "Division des données d’entête"
WakeOnLinkUp             = "Réveil sur liaison"
NumRssQueues             = "Nombre maximum de files d’attente RSS"
1Queue                   = "1 file d’attente"
2Queue                   = "2 files d’attente"
4Queue                   = "4 files d’attente"
IPSecv2                  = "Décharge IPsec"
AH                       = "Entête d’authentification activé"
ESP                      = "ESP activé"
AHESP                    = "Entête d’authentification & ESP activés"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; German
[Strings.0407]
Killer                  = "Killer"
AutoDetect               = "Autom. Aushandlung"
SpeedDuplex              = "Geschwindigkeit & Duplex"
10Mb-Half-Duplex         = "10 Mbit/s Halbduplex"
10Mb-Full-Duplex         = "10 Mbit/s Vollduplex"
100Mb-Half-Duplex        = "100 Mbit/s Halbduplex"
100Mb-Full-Duplex        = "100 Mbit/s Vollduplex"
1000Mb-Full-Duplex       = "1.0 Gbit/s Vollduplex"
2.5Gb-Full-Duplex        = "2.5 Gbit/s Vollduplex"
NetworkAddress           = "Netzwerkadresse"
IPChksumOffv4            = "IPv4 Prüfsummenabladung"
TCPChksumOffv4           = "TCP Prüfsummenabladung (IPv4)"
UDPChksumOffv4           = "UDP Prüfsummenabladung (IPv4)"
TCPChksumOffv6           = "TCP Prüfsummenabladung (IPv6)"
UDPChksumOffv6           = "UDP-Prüfsummenabladung (IPv6)"
Enabled                  = "Aktiviert"
Disabled                 = "Deaktiviert"
TxEnabled                = "Tx aktiviert"
RxEnabled                = "Rx deaktiviert"
RxTxEnabled              = "Rx & Tx aktiviert"
LSOv4                    = "Abladung großer Übertragung (IPv4)"
LSOv2v4                  = "Abladung großer Übertragung V2 (IPv4)"
LSOv2v6                  = "Abladung großer Übertragung V2 (IPv6)"
FlowControl              = "Fließkontrolle"
PriorityVLAN             = "Priorität & VLAN"
PriorityVLANDisabled     = "Priorität & VLAN deaktiviert"
PriorityVLANEnabled      = "Priorität & VLAN aktiviert"
InterruptModeration      = "Interrupt-Moderation"
ReceiveBuffers           = "Puffer empfangen"
TransmitBuffers          = "Puffer übertragen"
AutoDisableGigabit       = "Gigabit autom. deaktivieren"
AutoLinkDownPhyOff       = "PHY autom. deaktivieren"
BatteryRe-Link           = "Wiederverbindung, Batterie"
AcBatteryRe-Link         = "Wiederverbindung, Batterie oder Netz"
Battery                  = "Aktiviert, Batterie"
AcBattery                = "Aktiviert, Batterie oder Netz"
JumboFrame               = "Jumbo-Rahmen"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Wake-On-Lan herunterfahren"
AutoLinkDownPcieMacOff   = "PCIe autom. deaktivieren"
RSS                      = "Seitenskalierung empfangen"
AutoCrossoverDet         = "Autom. Crossover-Erkennung"
PriorityEnabled          = "Priorität aktiviert"
VLANEnabled              = "VLAN aktiviert"
10MbFirst                = "10 Mbit/s zuerst"
100MbFirst               = "100 Mbit/s zuerst"
WolShutdownLinkSpeed     = "WoL / Link-Geschwindigkeit reduzieren"
NotSpeedDown             = "Nicht verlangsamen"
WolCap                   = "Wake-On-LAN-Funktionen"
None                     = "Kein"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Green-Ethernet"
WakeOnPtn                = "Bei Musterübereinstimmung aufwecken"
WakeOnMagPkt             = "Bei Magic Packet aufwecken"
ARPOffload               = "ARP-Abladen"
NsOffload                = "NS-Abladen"
EEE                      = "Energy-Efficient Ethernet (LAN-Energiesparen, EEE)"
HDSplit                  = "Header-Datenaufteilung"
WakeOnLinkUp             = "Bei Verbindung aufwecken"
NumRssQueues             = "Maximale RSS-Warteschlangenanzahl"
1Queue                   = "1 Warteschlange"
2Queue                   = "2 Warteschlangen"
4Queue                   = "4 Warteschlangen"
IPSecv2                  = "IPsec-Abladen"
AH                       = "Auth Header aktiviert"
ESP                      = "ESP aktiviert"
AHESP                    = "Auth Header & ESP aktiviert"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Greek
[Strings.0408]
Killer                  = "Killer"
AutoDetect               = "Αυτόματη διαπραγμάτευση"
SpeedDuplex              = "Ταχύτητα & Αμφίδρομη"
10Mb-Half-Duplex         = "10Mbps/Ημι-αμφίδρομη"
10Mb-Full-Duplex         = "10Mbps/Πλήρως αμφίδρομη"
100Mb-Half-Duplex        = "100Mbps/Ημι-αμφίδρομη"
100Mb-Full-Duplex        = "100Mbps/Πλήρως αμφίδρομη"
1000Mb-Full-Duplex       = "1.0Gbps/Πλήρως αμφίδρομη"
2.5Gb-Full-Duplex        = "2.5Gbps/Πλήρως αμφίδρομη"
NetworkAddress           = "Διεύθυνση δικτύου"
IPChksumOffv4            = "Μείωση φόρτου αθροίσματος ελέγχου IPv4"
TCPChksumOffv4           = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv4)"
UDPChksumOffv4           = "Μείωση φόρτου αθροίσματος ελέγχου UDP (IPv4)"
TCPChksumOffv6           = "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv6)"
UDPChksumOffv6           = "Μείωση φόρτου αθροίσματος ελέγχου UDP (IPv6)"
Enabled                  = "Ενεργοποιημένο"
Disabled                 = "Απενεργοποιημένο"
TxEnabled                = "Ενεργοποιημένο Tx"
RxEnabled                = "Ενεργοποιημένο Rx"
RxTxEnabled              = "Ενεργοποιημένο Rx & Tx"
LSOv4                    = "Μείωση φόρτου μεγάλης αποστολής (IPv4)"
LSOv2v4                  = "Μείωση φόρτου μεγάλης αποστολής v2 (IPv4)"
LSOv2v6                  = "Μείωση φόρτου μεγάλης αποστολής v2 (IPv6)"
FlowControl              = "Έλεγχος ροής"
PriorityVLAN             = "Προτεραιότητα & VLAN"
PriorityVLANDisabled     = "Απενεργοποίηση προτεραιότητας & VLAN"
PriorityVLANEnabled      = "Ενεργοποίηση προτεραιότητας & VLAN"
InterruptModeration      = "Διακοπή επόπτευσης"
ReceiveBuffers           = "Προσωρινοί χώροι παραλαβής"
TransmitBuffers          = "Προσωρινοί χώροι μετάδοσης"
AutoDisableGigabit       = "Gigabit αυτόματης απενεργοποίησης"
AutoLinkDownPhyOff       = "PHY αυτόματης απενεργοποίησης"
BatteryRe-Link           = "Επανασύνδεση, Μπαταρία"
AcBatteryRe-Link         = "Επανασύνδεση, Μπαταρία ή AC"
Battery                  = "Ενεργοποίηση, Μπαταρία"
AcBattery                = "Ενεργοποίηση, Μπαταρία ή AC"
JumboFrame               = "Πλαίσιο Jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Wake-on-LAN τερματισμού"
AutoLinkDownPcieMacOff   = "PCIe αυτόματης απενεργοποίησης"
RSS                      = "Παραλαβή πλευρικής κλιμάκωσης"
AutoCrossoverDet         = "Αυτόματη ανίχνευση τιμής διασταύρωσης"
PriorityEnabled          = "Ενεργοποίηση προτεραιότητας"
VLANEnabled              = "Ενεργοποίηση VLAN"
10MbFirst                = "Πρώτα 10 Mbps"
100MbFirst               = "Πρώτα 100 Mbps"
WolShutdownLinkSpeed     = "Ταχύτητα σύνδεσης τερματισμού & WOL"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Ενεργοποίηση με αντιστοίχιση μοτίβου"
WakeOnMagPkt             = "Ενεργοποίηση με Μαγικό πακέτο"
ARPOffload               = "Μείωση φόρτου ARP"
NsOffload                = "Μείωση φόρτου NS"
EEE                      = "Ethernet με αποτελεσματική χρήση ενέργειας"
HDSplit                  = "Διαίρεση δεδομένων κεφαλίδας"
WakeOnLinkUp             = "Ενεργοποίηση κατά τη σύνδεση"
NumRssQueues             = "Μέγιστος αριθμός ουρών RSS"
1Queue                   = "1 ουρά"
2Queue                   = "2 ουρές"
4Queue                   = "4 ουρές"
IPSecv2                  = "Μείωση φόρτου IPsec"
AH                       = "Η κεφαλίδα ελέγχου ταυτότητας έχει ενεργοποιηθεί"
ESP                      = "Το ESP έχει ενεργοποιηθεί"
AHESP                    = "Η κεφαλίδα ελέγχου ταυτότητας & το ESP έχουν ενεργοποιηθεί"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Hebrew
[Strings.040D]
Killer                  = "Killer"
AutoDetect               = "משא ומתן אוטומטי"
SpeedDuplex              = "מהירות וכיווניות"
10Mb-Half-Duplex         = "10Mbps חד כיווני"
10Mb-Full-Duplex         = "10Mbps דו כיווני"
100Mb-Half-Duplex        = "100Mbps חד כיווני"
100Mb-Full-Duplex        = "100Mbps דו כיווני"
1000Mb-Full-Duplex       = "1000Mbps דו כיווני"
2.5Gb-Full-Duplex        = "2500Mbps דו כיווני"
NetworkAddress           = "כתובת רשת"
IPChksumOffv4            = "העברת סיכום ביקורת IPv4"
TCPChksumOffv4           = "העברת סיכום ביקורת IPv4) TCP)"
UDPChksumOffv4           = "העברת סיכום ביקורת IPv4) UDP)"
TCPChksumOffv6           = "העברת סיכום ביקורת IPv6) TCP)"
UDPChksumOffv6           = "העברת סיכום ביקורת IPv6) UDP)"
Enabled                  = "מאופשר"
Disabled                 = "מבוטל"
TxEnabled                = "שידור מאופשר"
RxEnabled                = "קליטה מאופשרת"
RxTxEnabled              = "שידור וקליטה מאופשרים"
LSOv4                    = "העברת שליחה גדולה (IPv4)"
LSOv2v4                  = "העברת שליחה גדולה IPv4) v2)"
LSOv2v6                  = "העברת שליחה גדולה IPv6) v2)"
FlowControl              = "בקרת זרימה"
PriorityVLAN             = "עדיפות ו-VLAN"
PriorityVLANDisabled     = "עדיפות ו-VLAN מבוטלות"
PriorityVLANEnabled      = "עדיפות ו-VLAN מאופשרות"
InterruptModeration      = "צמצום פסיקות"
ReceiveBuffers           = "מאגרי קליטה"
TransmitBuffers          = "מאגרי שידור"
AutoDisableGigabit       = "ביטול אוטומטי של PowerSaving) Gigabit)"
AutoLinkDownPhyOff       = "ביטול אוטומטי של PowerSaving) PHY)"
BatteryRe-Link           = "קישור מחדש, סוללה"
AcBatteryRe-Link         = "קישור מחדש, סוללה או מתח חילופין (AC)"
Battery                  = "מאופשר, סוללה"
AcBattery                = "מאופשר, סוללה או מתח חילופין (AC)"
JumboFrame               = "מסגרת Jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "כיבוי Wake-On-Lan"
AutoLinkDownPcieMacOff   = "ביטול אוטומטי של PowerSaving) PCIe)"
RSS                      = "התאמת גודל בצד הקליטה"
AutoCrossoverDet         = "גילוי אוטומטי של חיבור מוצלב"
PriorityEnabled          = "עדיפות מאופשרת"
VLANEnabled              = "VLAN מאופשר"
10MbFirst                = "10Mbps ראשון"
100MbFirst               = "100Mbps ראשון"
WolShutdownLinkSpeed     = "מהירות קישור כיבוי ו-WOL"
NotSpeedDown             = "ללא האטה"
WolCap                   = "יכולות Wake-On-Lan"
None                     = "ללא"
PatternMatch             = "התאמת תבנית"
MagicPacket              = "מנת קסם"
PatternAndMagic          = "התאמת תבנית ומנת קסם"
GreenEthernet            = "ירוקEthernet"
WakeOnPtn                = "התאמת תבנית התעוררות"
WakeOnMagPkt             = "Magic Packet של התעוררות"
ARPOffload               = "העברת פרוטוקול ARP (פרוטוקול מציאת כתובת)"
NsOffload                = "העברת בקשת NS (בקשת זיהוי של שכן)"
EEE                      = "אתרנט חסכוני בחשמל"
HDSplit                  = "פיצול נתוני כותרת"
WakeOnLinkUp             = "קישור להתעוררות"
NumRssQueues             = "המספר המרבי של תורי RSS (שינוי קנה מידה של הצד המקבל)"
1Queue                   = "תור אחד"
2Queue                   = "2 תורים"
4Queue                   = "4 תורים"
IPSecv2                  = "העברת אבטחת IP (פרוטוקול אינטרנט)"
AH                       = "כותרת אימות הופעלה"
ESP                      = "ESP הופעל (אריזת נתוני אבטחה)"
AHESP                    = "כותרת אימות ו- ESP הופעלו"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Hungarian
[Strings.040e]
Killer                  = "Killer"
AutoDetect               = "Automatikus sebesség- és duplexitás-felismerés"
SpeedDuplex              = "Sebesség és duplex"
10Mb-Half-Duplex         = "10 Mbps Félduplex"
10Mb-Full-Duplex         = "10 Mbps Teljes duplex"
100Mb-Half-Duplex        = "100 Mbps Mbps Félduplex"
100Mb-Full-Duplex        = "100 Mbps Teljes duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Teljes duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Teljes duplex"
NetworkAddress           = "Hálózati cím"
IPChksumOffv4            = "IPv4 Ellenőrzőösszeg tehermentesítése"
TCPChksumOffv4           = "TCP Ellenőrzőösszeg tehermentesítése (IPv4)"
UDPChksumOffv4           = "UDP Ellenőrzőösszeg tehermentesítése (IPv4)"
TCPChksumOffv6           = "TCP Ellenőrzőösszeg tehermentesítése (IPv6)"
UDPChksumOffv6           = "UDP Ellenőrzőösszeg tehermentesítése (IPv6)"
Enabled                  = "Engedélyezve"
Disabled                 = "Letiltva"
TxEnabled                = "Tx Engedélyezve"
RxEnabled                = "Rx Engedélyezve"
RxTxEnabled              = "Rx és Tx Engedélyezve"
LSOv4                    = "Nagyobb küldemény tehermentesítése (IPv4)"
LSOv2v4                  = "Nagyobb küldemény tehermentesítése v2 (IPv4)"
LSOv2v6                  = "Nagyobb küldemény tehermentesítése v2 (IPv6)"
FlowControl              = "Áramlásszabályozás"
PriorityVLAN             = "Prioritás és VLAN"
PriorityVLANDisabled     = "Prioritás és VLAN letiltva"
PriorityVLANEnabled      = "Prioritás és VLAN engedélyezve"
InterruptModeration      = "Megszakítás visszatartása"
ReceiveBuffers           = "Vételi pufferek"
TransmitBuffers          = "Átviteli pufferek"
AutoDisableGigabit       = "Gigabit automatikus letiltása"
AutoLinkDownPhyOff       = "PHY automatikus letiltása"
BatteryRe-Link           = "Újrakapcsolódás, akkumulátor"
AcBatteryRe-Link         = "Újrakapcsolódás, akkumulátor vagy AC"
Battery                  = "Engedélyezve, akkumulátor"
AcBattery                = "Engedélyezve, akkumulátor vagy AC"
JumboFrame               = "Jumbo Frame (Óriás keret)"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Felélesztés leállítás után hálózaton keresztül"
AutoLinkDownPcieMacOff   = "PCIe automatikus letiltása"
RSS                      = "Vételoldali skálázás"
AutoCrossoverDet         = "Keresztezés automatikus észlelése"
PriorityEnabled          = "Prioritás engedélyezve"
VLANEnabled              = "VLAN engedélyezve"
10MbFirst                = "10 Mbps/Első"
100MbFirst               = "100 Mbps/Első"
WolShutdownLinkSpeed     = "WOL és leállítás kapcsolati sebessége"
NotSpeedDown             = "Nincs lassítás"
WolCap                   = "Hálózaton keresztül történő felélesztéssel kapcsolatos funkciók"
None                     = "Nincs"
PatternMatch             = "Mintaillesztés"
MagicPacket              = "Megfelelő csomag"
PatternAndMagic          = "Mintaillesztés és megfelelő csomag"
GreenEthernet            = "Energiatakarékos Ethernet"
WakeOnPtn                = "Ébresztés egyező mintára"
WakeOnMagPkt             = "Ébresztés Magic Packetre"
ARPOffload               = "ARP lerakodás"
NsOffload                = "NS lerakodás"
EEE                      = "Energia-hatékony Ethernet"
HDSplit                  = "Fejlécadatok felosztása"
WakeOnLinkUp             = "Ébresztés csatlakozásra"
NumRssQueues             = "RSS várakozási sorok maximális száma"
1Queue                   = "1 sor"
2Queue                   = "2 sor"
4Queue                   = "4 sor"
IPSecv2                  = "IPsec lerakodás"
AH                       = "Hitelesítő fejléc engedélyezve"
ESP                      = "ESP engedélyezve"
AHESP                    = "Hitelesítő fejléc és ESP engedélyezve"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Italian
[Strings.0410]
Killer                  = "Killer"
AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Velocità e duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Indirizzo di rete"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Abilitato"
Disabled                 = "Disabilitato"
TxEnabled                = "Tx Abilitata"
RxEnabled                = "Rx Abilitata"
RxTxEnabled              = "Rx & Tx Abilitata"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Controllo flusso"
PriorityVLAN             = "Priorità e VLAN"
PriorityVLANDisabled     = "Priorità e VLAN disabilitata"
PriorityVLANEnabled      = "Priorità e VLAN abilitata"
InterruptModeration      = "Interrupt Moderation"
ReceiveBuffers           = "Ricevi buffer"
TransmitBuffers          = "Trasmetti buffer"
AutoDisableGigabit       = "Disabilitazione automatica gigabit"
AutoLinkDownPhyOff       = "Disabilitazione automatica PHY"
BatteryRe-Link           = "Ricollegamento, batteria"
AcBatteryRe-Link         = "Ricollegamento, batteria o AC"
Battery                  = "Abilitato, batteria"
AcBattery                = "Abilitato, batteria o AC"
JumboFrame               = "Jumbo Frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Disabilitazione automatica PCIe"
RSS                      = "Ricevi side scaling"
AutoCrossoverDet         = "Rilevamento automatico crossover"
PriorityEnabled          = "Priorità abilitata"
VLANEnabled              = "VLAN abilitata"
10MbFirst                = "Prima 10 Mbps"
100MbFirst               = "Prima 100 Mbps"
WolShutdownLinkSpeed     = "WOL & Shutdown velocità collegamento"
NotSpeedDown             = "Non rallentamento"
WolCap                   = "Funzioni Wake-On-Lan"
None                     = "Nessuno"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match e Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Corrispondenza motivo per riattivazione"
WakeOnMagPkt             = "Magic Packet per riattivazione"
ARPOffload               = "Offload ARP"
NsOffload                = "Offload NS"
EEE                      = "Ethernet a risparmio energetico"
HDSplit                  = "Separazione dati intestazioni"
WakeOnLinkUp             = "Collegamento per riattivazione"
NumRssQueues             = "Numero massimo code RSS"
1Queue                   = "1 coda"
2Queue                   = "2 code"
4Queue                   = "4 code"
IPSecv2                  = "Offload IPSec"
AH                       = "Intestazione autent. attivata"
ESP                      = "ESP attivato"
AHESP                    = "Intestazione autent. ed ESP attivati"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Japanese
[Strings.0411]
Killer                  = "Killer"
AutoDetect               = "自動ネゴシエーション"
SpeedDuplex              = "速度とデュプレックス"
10Mb-Half-Duplex         = "10 Mbps ハーフデュプレックス"
10Mb-Full-Duplex         = "10 Mbps フルデュプレックス"
100Mb-Half-Duplex        = "100 Mbps ハーフデュプレックス"
100Mb-Full-Duplex        = "100 Mbps フルデュプレックス"
1000Mb-Full-Duplex       = "1.0 Gbps フルデュプレックス"
2.5Gb-Full-Duplex        = "2.5 Gbps フルデュプレックス"
NetworkAddress           = "ネットワークアドレス"
IPChksumOffv4            = "IPv4 チェックサムオフロード"
TCPChksumOffv4           = "TCP チェックサムオフロード (IPv4)"
UDPChksumOffv4           = "UDP チェックサムオフロード (IPv4)"
TCPChksumOffv6           = "TCP チェックサムオフロード (IPv6)"
UDPChksumOffv6           = "UDP チェックサムオフロード (IPv6)"
Enabled                  = "有効"
Disabled                 = "無効"
TxEnabled                = "Tx 有効"
RxEnabled                = "Rx 有効"
RxTxEnabled              = "受信と伝送有効"
LSOv4                    = "一括送信オフロード (IPv4)"
LSOv2v4                  = "一括送信オフロード v2 (IPv4)"
LSOv2v6                  = "一括送信オフロード v2 (IPv6)"
FlowControl              = "フローコントロール"
PriorityVLAN             = "優先度およびVLAN"
PriorityVLANDisabled     = "優先度およびVLAN 無効"
PriorityVLANEnabled      = "優先度およびVLAN 有効"
InterruptModeration      = "割込みモデレーション"
ReceiveBuffers           = "受信バッファ"
TransmitBuffers          = "伝送バッファ"
AutoDisableGigabit       = "自動無効ギガビット"
AutoLinkDownPhyOff       = "自動無効PHY"
BatteryRe-Link           = "再リンク、バッテリ"
AcBatteryRe-Link         = "再リンク、バッテリまたはAC"
Battery                  = "有効、バッテリ"
AcBattery                = "有効、バッテリまたはAC"
JumboFrame               = "ジャンボフレーム"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "LAN 上のウェークアップのシャットダウン"
AutoLinkDownPcieMacOff   = "自動無効 PCIe"
RSS                      = "受信側スケーリング"
AutoCrossoverDet         = "自動クロスオーバー検出"
PriorityEnabled          = "優先度有効"
VLANEnabled              = "VLAN 有効"
10MbFirst                = "10 Mbps 優先"
100MbFirst               = "100 Mbps 優先"
WolShutdownLinkSpeed     = "WOL とシャットダウンリンク速度"
NotSpeedDown             = "速度低下ではない"
WolCap                   = "Wake-On-Lan機能"
None                     = "なし"
PatternMatch             = "パターン適合"
MagicPacket              = "マジックパケット"
PatternAndMagic          = "パターン適合とマジックパケット"
GreenEthernet            = "グリーンイーサネット"
WakeOnPtn                = "ウェイク・オン・パターン・マッチ"
WakeOnMagPkt             = "ウェイク・オン・マジック・パケット"
ARPOffload               = "ARP オフロード"
NsOffload                = "NS オフロード"
EEE                      = "省電力型イーサネット(EEE)"
HDSplit                  = "ヘッダーデータ分割"
WakeOnLinkUp             = "ウェイクオン結合"
NumRssQueues             = "RSSキューの最大数"
1Queue                   = "1キュー"
2Queue                   = "2キュー"
4Queue                   = "4キュー"
IPSecv2                  = "IPsecアンロード"
AH                       = "Authヘッダーの有効"
ESP                      = "ESPの有効"
AHESP                    = "AuthヘッダーとESPの有効"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Korean
[Strings.0412]
Killer                  = "Killer"
AutoDetect               = "자동 교섭"
SpeedDuplex              = "속도 및 이중"
10Mb-Half-Duplex         = "10 Mbps 반이중"
10Mb-Full-Duplex         = "10 Mbps 전이중"
100Mb-Half-Duplex        = "100 Mbps 반이중"
100Mb-Full-Duplex        = "100 Mbps 전이중"
1000Mb-Full-Duplex       = "1.0 Gbps 전이중"
2.5Gb-Full-Duplex        = "2.5 Gbps 전이중"
NetworkAddress           = "네트워크 주소"
IPChksumOffv4            = "IPv4 체크섬 오프로드"
TCPChksumOffv4           = "TCP 체크섬 오프로드(IPv4)"
UDPChksumOffv4           = "UDP 체크섬 오프로드(IPv4)"
TCPChksumOffv6           = "TCP 체크섬 오프로드(IPv6)"
UDPChksumOffv6           = "UDP 체크섬 오프로드(IPv6)"
Enabled                  = "사용"
Disabled                 = "사용 안 함"
TxEnabled                = "Tx 사용"
RxEnabled                = "Rx 사용"
RxTxEnabled              = "Rx/Tx 사용"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "흐름 제어"
PriorityVLAN             = "우선 순위 및 VLAN"
PriorityVLANDisabled     = "우선 순위 및 VLAN 사용 안 함"
PriorityVLANEnabled      = "우선 순위 및 VLAN 사용"
InterruptModeration      = "인터럽트 완화"
ReceiveBuffers           = "수신 버퍼"
TransmitBuffers          = "송신 버퍼"
AutoDisableGigabit       = "Gigabit 자동 비활성화(절전)"
AutoLinkDownPhyOff       = "PHY 자동 비활성화(절전)"
BatteryRe-Link           = "다시 연결, 전지"
AcBatteryRe-Link         = "다시 연결, 전지 또는 AC"
Battery                  = "사용, 전지"
AcBattery                = "사용, 전지 또는 AC"
JumboFrame               = "점보 프레임"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "웨이크 온 랜 종료"
AutoLinkDownPcieMacOff   = "PCIe 자동 비활성화(절전)"
RSS                      = "수신측 조정"
AutoCrossoverDet         = "자동 크로스오버 탐지"
PriorityEnabled          = "우선 순위 사용"
VLANEnabled              = "VLAN 사용"
10MbFirst                = "10 Mbps 먼저"
100MbFirst               = "100 Mbps 먼저"
WolShutdownLinkSpeed     = "WOL 및 종료 링크 속도"
NotSpeedDown             = "속도 저하 안 함"
WolCap                   = "WOL 기능"
None                     = "없음"
PatternMatch             = "패턴 매치"
MagicPacket              = "매직 패킷"
PatternAndMagic          = "패턴 매치와 매직 패킷"
GreenEthernet            = "절전형 이더넷"
WakeOnPtn                = "패턴 일치 웨이크 온"
WakeOnMagPkt             = "매직 패킷 웨이크 온"
ARPOffload               = "ARP 오프로드"
NsOffload                = "NS 오프로드"
EEE                      = "에너지 효율적인 이더넷"
HDSplit                  = "헤더 데이터 분할"
WakeOnLinkUp             = "링크 업 웨이크 온"
NumRssQueues             = "RSS 대기행렬의 최대 수"
1Queue                   = "1개의 대기행렬"
2Queue                   = "2개의 대기행렬"
4Queue                   = "4개의 대기행렬"
IPSecv2                  = "IPsec 오프로드"
AH                       = "인증 헤더가 활성화됨"
ESP                      = "ESP가 활성화됨"
AHESP                    = "인증 헤더와ㅜESP가 활성화됨"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Norwegian_Bokmal
[Strings.0414]
Killer                  = "Killer"
AutoDetect               = "Automatisk forhandling"
SpeedDuplex              = "Hastighet og dupleks"
10Mb-Half-Duplex         = "10Mbps Halv dupleks"
10Mb-Full-Duplex         = "10Mbps Full dupleks"
100Mb-Half-Duplex        = "100Mbps Halv dupleks"
100Mb-Full-Duplex        = "100Mbps Full dupleks"
1000Mb-Full-Duplex       = "1.0Gbps Full dupleks"
2.5Gb-Full-Duplex        = "2.5Gbps Full dupleks"
NetworkAddress           = "Nettverksadresse"
IPChksumOffv4            = "IPv4 Sjekksum avlastning"
TCPChksumOffv4           = "TCP Sjekksum avlastning (IPv4)"
UDPChksumOffv4           = "UDP Sjekksum avlastning (IPv4)"
TCPChksumOffv6           = "TCP Sjekksum avlastning (Ipv6)"
UDPChksumOffv6           = "UDP Sjekksum avlastning (Ipv6)"
Enabled                  = "Aktivert"
Disabled                 = "Deaktivert"
TxEnabled                = "Tx aktivert"
RxEnabled                = "Rx aktivert"
RxTxEnabled              = "Rx og Tx aktivert"
LSOv4                    = "Stor sending avlastning (IPv4)"
LSOv2v4                  = "Stor sending avlastning v2 (IPv4)"
LSOv2v6                  = "Stor sending avlastning v2 (Ipv6)"
FlowControl              = "Flytkontroll"
PriorityVLAN             = "Prioritet og VLAN"
PriorityVLANDisabled     = "Prioritet og VLAN deaktivert"
PriorityVLANEnabled      = "Prioritet og VLAN aktivert"
InterruptModeration      = "Avbruddsmoderering"
ReceiveBuffers           = "Mottaksbuffere"
TransmitBuffers          = "Sendebuffere"
AutoDisableGigabit       = "Automatisk deaktivere gigabit"
AutoLinkDownPhyOff       = "Automatisk deaktivere PHY"
BatteryRe-Link           = "Ny linje, batteri"
AcBatteryRe-Link         = "Ny linje, batteri eller vekselstrøm"
Battery                  = "Aktivert, batteri"
AcBattery                = "Aktivert, batteri or vekselstrøm"
JumboFrame               = "Jumbo-ramme"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Avslutningsaktivering på nettverk"
AutoLinkDownPcieMacOff   = "Automatisk deaktivere PCIe"
RSS                      = "Mottak sideskalering"
AutoCrossoverDet         = "Automatisk registrering av grenbytte"
PriorityEnabled          = "Prioritet aktivert"
VLANEnabled              = "VLAN aktivert"
10MbFirst                = "10 Mbps Først"
100MbFirst               = "100 Mbps Først"
WolShutdownLinkSpeed     = "WOL og avslutningslinjehastighet"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Grønt Ethernet"
WakeOnPtn                = "Reaktiver når mønster samsvarer"
WakeOnMagPkt             = "Reaktivert etter magisk pakke"
ARPOffload               = "ARP-avlasting"
NsOffload                = "NS-avlasting"
EEE                      = "Energy-Efficient Ethernet"
HDSplit                  = "Oppdeling av hodedata"
WakeOnLinkUp             = "Våkne ved oppkobling"
NumRssQueues             = "Maksimalt antall RSS-køer"
1Queue                   = "1 kø"
2Queue                   = "2 køer"
4Queue                   = "4 køer"
IPSecv2                  = "IPsec-avlasting"
AH                       = "Godkj.hode aktivert"
ESP                      = "ESP aktivert"
AHESP                    = "Godkj.hode og ESP aktivert"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Polish
[Strings.0415]
Killer                  = "Killer"
AutoDetect               = "Automatyczne negocjacje"
SpeedDuplex              = "Szybkość i dupleks"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Adres sieciowy"
IPChksumOffv4            = "Suma kontrolna bez obciążenia IPv4"
TCPChksumOffv4           = "Suma kontrolna bez obciążenia TCP (IPv4)"
UDPChksumOffv4           = "Suma kontrolna bez obciążenia UDP (IPv4)"
TCPChksumOffv6           = "Suma kontrolna bez obciążenia TCP (IPv6)"
UDPChksumOffv6           = "Suma kontrolna bez obciążenia UDP (IPv6)"
Enabled                  = "Włączone"
Disabled                 = "Wyłączone"
TxEnabled                = "Włączone Tx"
RxEnabled                = "Włączone Rx"
RxTxEnabled              = "Włączone Rx i Tx"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Sterowanie przepływem"
PriorityVLAN             = "Priorytet i VLAN"
PriorityVLANDisabled     = "Wyłączony Priorytet i VLAN"
PriorityVLANEnabled      = "Włączony Priorytet i VLAN"
InterruptModeration      = "Moderacja przerwania"
ReceiveBuffers           = "Bufory odbioru"
TransmitBuffers          = "Bufory transmisji"
AutoDisableGigabit       = "Automatyczne wyłączanie Gigabit"
AutoLinkDownPhyOff       = "Automatyczne wyłączanie PHY"
BatteryRe-Link           = "Ponowne podłączenie, bateria"
AcBatteryRe-Link         = "Ponowne podłączenie, bateria lub prąd zmienny"
Battery                  = "Włączone, bateria"
AcBattery                = "Włączone, bateria lub prąd zmienny"
JumboFrame               = "Ramka Jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Zamknięcie Wybudzanie przy uaktywnieniu sieci"
AutoLinkDownPcieMacOff   = "Automatyczne wyłączenie PCIe"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Autodetekcja rodzaju połączenia"
PriorityEnabled          = "Włączony priorytet"
VLANEnabled              = "Włączona sieć VLAN"
10MbFirst                = "Najpierw 10 Mbps"
100MbFirst               = "Najpierw 100 Mbps"
WolShutdownLinkSpeed     = "WOL i szybkość zamykania łącza"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Energooszczędny Ethernet"
WakeOnPtn                = "Dopasowanie do wzorca wybudzania"
WakeOnMagPkt             = "Pakiet wybudzania Magic Packet"
ARPOffload               = "Rozładowanie ARP"
NsOffload                = "Rozładowanie NS"
EEE                      = "Ethernet efektywny energetycznie"
HDSplit                  = "Podział danych nagłówka"
WakeOnLinkUp             = "Uruchomienie łącza wybudzania"
NumRssQueues             = "Maksymalna liczba kolejek RSS"
1Queue                   = "1 kolejka"
2Queue                   = "2 kolejki"
4Queue                   = "4 kolejki"
IPSecv2                  = "Rozładowanie IPsec"
AH                       = "Włączony nagłówek uwierzytelniania"
ESP                      = "Włączone ESP"
AHESP                    = "Włączony nagłówek uwierzytelniania i ESP"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Portuguese_Brazilian
[Strings.0416]
Killer                  = "Killer"
AutoDetect               = "Auto Negociação"
SpeedDuplex              = "Velocidade & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Endereço de Rede"
IPChksumOffv4            = "IPv4 Descarga de Checksum"
TCPChksumOffv4           = "TCP Descarga de Checksum (IPv4)"
UDPChksumOffv4           = "UDP Descarga de Checksum (IPv4)"
TCPChksumOffv6           = "TCP Descarga de Checksum (IPv6)"
UDPChksumOffv6           = "UDP Descarga de Checksum (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Tx Activado"
RxEnabled                = "Rx Activado"
RxTxEnabled              = "Rx & Tx Activados"
LSOv4                    = "Descarga Large Send (IPv4)"
LSOv2v4                  = "Descarga Large Send v2 (IPv4)"
LSOv2v6                  = "Descarga Large Send v2 (IPv6)"
FlowControl              = "Controlo de Fluxo"
PriorityVLAN             = "Prioridade & VLAN"
PriorityVLANDisabled     = "Prioridade & VLAN Desactivados"
PriorityVLANEnabled      = "Prioridade & VLAN Activados"
InterruptModeration      = "Moderação de Interrupção"
ReceiveBuffers           = "Receber Memórias Intermédias"
TransmitBuffers          = "Transmitir Memórias Intermédias"
AutoDisableGigabit       = "Auto Desactivar Gigabit"
AutoLinkDownPhyOff       = "Auto Desactivar PHY"
BatteryRe-Link           = "Re-Ligar, Bateria"
AcBatteryRe-Link         = "Re-Ligar, Bateria ou AC"
Battery                  = "Activado, Bateria"
AcBattery                = "Activado, Bateria ou CA"
JumboFrame               = "Jumbo Frame"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Desligar Despertar Aquando de Lan"
AutoLinkDownPcieMacOff   = "Auto Desactivar PCIe"
RSS                      = "Receber Side Scaling"
AutoCrossoverDet         = "Detecção Auto Crossover"
PriorityEnabled          = "Prioridade Activada"
VLANEnabled              = "VLAN Activada"
10MbFirst                = "10 Mbps Primeiro"
100MbFirst               = "100 Mbps Primeiro"
WolShutdownLinkSpeed     = "WOL & Desligar Velocidade Ligação"
NotSpeedDown             = "Não reduzir velocidade"
WolCap                   = "Capacidades Wake-On-Lan"
None                     = "Nenhum"
PatternMatch             = "Correspondência de padrões"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Correspondência de pacotes e Magic Packet"
GreenEthernet            = "Ethernet Verde"
WakeOnPtn                = "Combinação do padrão Wake on"
WakeOnMagPkt             = "Pacote Wake on Magic"
ARPOffload               = "Transferência ARP"
NsOffload                = "Transferência NS"
EEE                      = "Energia Eficiente Ethernet"
HDSplit                  = "Separação de Dados do Título"
WakeOnLinkUp             = "Ligação de Wake On"
NumRssQueues             = "Número Máximo de Filas RSS"
1Queue                   = "1 Fila"
2Queue                   = "2 Filas"
4Queue                   = "4 Filas"
IPSecv2                  = "Transferência IPsec"
AH                       = "Autent Título Ativado"
ESP                      = "ESP Ativado"
AHESP                    = "Autent Título & ESP Ativados"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Portuguese_Standard
[Strings.0816]
Killer                  = "Killer"
AutoDetect               = "Auto negociação"
SpeedDuplex              = "Velocidade e modo duplex"
10Mb-Half-Duplex         = "10 Mbps modo semi duplex"
10Mb-Full-Duplex         = "10 Mbps modo full-duplex"
100Mb-Half-Duplex        = "100 Mbps modo semi duplex"
100Mb-Full-Duplex        = "100 Mbps modo full-duplex"
1000Mb-Full-Duplex       = "1,0 Gbps modo full-duplex"
2.5Gb-Full-Duplex        = "2,5 Gbps modo full-duplex"
NetworkAddress           = "Endereço de rede"
IPChksumOffv4            = "Soma de verificação offload IPv4"
TCPChksumOffv4           = "Soma de verificação offload TCP (IPv4)"
UDPChksumOffv4           = "Soma de verificação offload UDP (IPv4)"
TCPChksumOffv6           = "Soma de verificação offload TCP (IPv6)"
UDPChksumOffv6           = "Soma de verificação offload UDP (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Transmissão activada"
RxEnabled                = "Recepção activada"
RxTxEnabled              = "Recepção e transmissão activada"
LSOv4                    = "Envio grande de offload (IPv4)"
LSOv2v4                  = "Envio grande de offload v2 (IPv4)"
LSOv2v6                  = "Envio grande de offload v2 (IPv6)"
FlowControl              = "Controlo do fluxo"
PriorityVLAN             = "Prioridade e VLAN"
PriorityVLANDisabled     = "Prioridade e VLAN desactivada"
PriorityVLANEnabled      = "Prioridade e VLAN activada"
InterruptModeration      = "Moderação de interrupção"
ReceiveBuffers           = "Memória de recepção"
TransmitBuffers          = "Memória de transmissão"
AutoDisableGigabit       = "Desactivar Gigabit automaticamente"
AutoLinkDownPhyOff       = "Desactivar PHY automaticamente"
BatteryRe-Link           = "Religar, bateria"
AcBatteryRe-Link         = "Religar, bateria ou a.c."
Battery                  = "Activada, bateria"
AcBattery                = "Activada, bateria ou a.c."
JumboFrame               = "Estrutura jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Encerrar Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Desactivar PCIe automaticamente"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Detecção cruzada automática"
PriorityEnabled          = "Prioridade activada"
VLANEnabled              = "VLAN activada"
10MbFirst                = "10 Mbps primeiro"
100MbFirst               = "100 Mbps primeiro"
WolShutdownLinkSpeed     = "WOL e encerrar velocidade de ligação"
NotSpeedDown             = "Não diminuir velocidade"
WolCap                   = "Capacidades Wake-On-Lan"
None                     = "Nenhuma"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match e Magic Packet"
GreenEthernet            = "Ethernet verde"
WakeOnPtn                = "Reactivação por correspondência de padrões"
WakeOnMagPkt             = "Reactivação por Magic Packet"
ARPOffload               = "Descarga de ARP"
NsOffload                = "Descarga de NS"
EEE                      = "Ethernet de Consumo de Energia Eficiente"
HDSplit                  = "Divisão de Dados do Cabeçalho"
WakeOnLinkUp             = "Reactivação por Ligação"
NumRssQueues             = "Número máximo de filas RSS"
1Queue                   = "1 Fila"
2Queue                   = "2 Filas"
4Queue                   = "4 Filas"
IPSecv2                  = "Descarga de IPsec"
AH                       = "Cabeçalho de Autenticação Activado"
ESP                      = "ESP Activado"
AHESP                    = "Cabeçalho de Autenticação e ESP Activados"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Romanian
[Strings.0418]
Killer                  = "Killer"
AutoDetect               = "Negociere automată"
SpeedDuplex              = "Viteză şi duplex"
10Mb-Half-Duplex         = "10 Mbps semiduplex"
10Mb-Full-Duplex         = "10 Mbps duplex"
100Mb-Half-Duplex        = "100 Mbps semiduplex"
100Mb-Full-Duplex        = "100 Mbps duplex"
1000Mb-Full-Duplex       = "1,0 Gbps duplex"
2.5Gb-Full-Duplex        = "2,5 Gbps duplex"
NetworkAddress           = "Adresă de reţea"
IPChksumOffv4            = "Preluare sarcină de verificare erori de transmisie IPv4"
TCPChksumOffv4           = "Preluare sarcină de verificare erori de transmisie TCP (IPv4)"
UDPChksumOffv4           = "Preluare sarcină de verificare erori de transmisie UDP(IPv4)"
TCPChksumOffv6           = "Preluare sarcină de verificare erori de transmisie TCP(IPv6)"
UDPChksumOffv6           = "Preluare sarcină de verificare erori de transmisie UDP (IPv6)"
Enabled                  = "Activat"
Disabled                 = "Dezactivat"
TxEnabled                = "Tx activat"
RxEnabled                = "Rx activat"
RxTxEnabled              = "Rx şi Tx activate"
LSOv4                    = "Preluare sarcină de trimitere pachete mari(IPv4)"
LSOv2v4                  = "Preluare sarcină de trimitere pachete mari v2 (IPv4)"
LSOv2v6                  = "Preluare sarcină de trimitere pachete mari v2 (IPv6)"
FlowControl              = "Control debit"
PriorityVLAN             = "Prioritate şi VLAN"
PriorityVLANDisabled     = "Prioritate şi VLAN dezactivate"
PriorityVLANEnabled      = "Prioritate şi VLAN activate"
InterruptModeration      = "Moderare întrerupere"
ReceiveBuffers           = "Zone tampon de primire"
TransmitBuffers          = "Zone tampon de trimitere"
AutoDisableGigabit       = "Dezactivare automată Gigabit"
AutoLinkDownPhyOff       = "Dezactivare automată PHY"
BatteryRe-Link           = "Reconectare, baterie"
AcBatteryRe-Link         = "Reconectare, baterie sau AC"
Battery                  = "Activat, baterie"
AcBattery                = "Activat, baterie sau AC"
JumboFrame               = "Cadru jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Închidere Trezire prin LAN"
AutoLinkDownPcieMacOff   = "Dezactivare automată PCIe"
RSS                      = "Primire scalare laterală"
AutoCrossoverDet         = "Detectare automată simulare modem"
PriorityEnabled          = "Prioritate activată"
VLANEnabled              = "VLAN activată"
10MbFirst                = "10 Mbps iniţial"
100MbFirst               = "100 Mbps iniţial"
WolShutdownLinkSpeed     = "WOL şi dezactivare viteză legătură"
NotSpeedDown             = "Fără reducere viteză"
WolCap                   = "Capacităţi trezire prin LAN"
None                     = "Niciun(a)"
PatternMatch             = "Potrivire obiecte"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Potrivire pachete şi Magic Packet"
GreenEthernet            = "Ethernet verde"
WakeOnPtn                = "Activare la potrivire model"
WakeOnMagPkt             = "Potrivire la pachet magic"
ARPOffload               = "Reducere sarcină protocol rezolvare adresă"
NsOffload                = "Reducere sarcină solicitare vecin"
EEE                      = "Ethernet eficient energetic"
HDSplit                  = "Divizare date antet"
WakeOnLinkUp             = "Activare la legătură disponibilă"
NumRssQueues             = "Număr maxim de cozi pentru scalare la primire"
1Queue                   = "1 coadă"
2Queue                   = "2 cozi"
4Queue                   = "4 cozi"
IPSecv2                  = "4 cozi"
AH                       = "Antet autentificare activat"
ESP                      = "Sarcină securitate încapsulare activată"
AHESP                    = "Antet autentificare şi sarcină securitate încapsulare activate"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Russian
[Strings.0419]
Killer                  = "Killer"
AutoDetect               = "Автосогласование"
SpeedDuplex              = "Скорость и дуплекс"
10Mb-Half-Duplex         = "10 Мбит/с полудуплекс"
10Mb-Full-Duplex         = "10 Мбит/с дуплекс"
100Mb-Half-Duplex        = "100 Мбит/с полудуплекс"
100Mb-Full-Duplex        = "100 Мбит/с дуплекс"
1000Mb-Full-Duplex       = "1 Гбит/с дуплекс"
2.5Gb-Full-Duplex        = "2.5 Гбит/с дуплекс"
NetworkAddress           = "Сетевой адрес"
IPChksumOffv4            = "Контрольная сумма разгрузки IPv4"
TCPChksumOffv4           = "Контрольная сумма разгрузки TCP (IPv4)"
UDPChksumOffv4           = "Контрольная сумма разгрузки UDP (IPv4)"
TCPChksumOffv6           = "Контрольная сумма разгрузки TCP (IPv6)"
UDPChksumOffv6           = "Контрольная сумма разгрузки UDP (IPv6)"
Enabled                  = "Вкл"
Disabled                 = "Выкл"
TxEnabled                = "Tx вкл"
RxEnabled                = "Rx вкл"
RxTxEnabled              = "Rx & Tx вкл"
LSOv4                    = "Разгрузка при большой отправке (IPv4)"
LSOv2v4                  = "Разгрузка при большой отправке v2 (IPv4)"
LSOv2v6                  = "Разгрузка при большой отправке v2 (IPv6)"
FlowControl              = "Управление потоком"
PriorityVLAN             = "Приоритет & VLAN"
PriorityVLANDisabled     = "Приоритет & VLAN выкл"
PriorityVLANEnabled      = "Приоритет & VLAN вкл"
InterruptModeration      = "Модерация прерывания"
ReceiveBuffers           = "Буферы приема"
TransmitBuffers          = "Буферы передачи"
AutoDisableGigabit       = "Автоотключение гигабитной скорости"
AutoLinkDownPhyOff       = "Автоотключение PHY"
BatteryRe-Link           = "Переподключение, батарея"
AcBatteryRe-Link         = "Переподключение, батарея или пер. ток"
Battery                  = "Вкл, батарея"
AcBattery                = "Вкл, батарея или пер. ток"
JumboFrame               = "Большой кадр"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Включение по локальной сети после отключения"
AutoLinkDownPcieMacOff   = "Автоотключение PCIe"
RSS                      = "Получение бокового масштабирования"
AutoCrossoverDet         = "Автоопределение кросс-кабеля"
PriorityEnabled          = "Приоритет вкл"
VLANEnabled              = "VLAN вкл"
10MbFirst                = "Сначала 10 Mбит/с"
100MbFirst               = "Сначала 100 Mбит/с"
WolShutdownLinkSpeed     = "Скорость при включении по локальной сети после отключения"
NotSpeedDown             = "Не использовать автопонижение скорости"
WolCap                   = "Функции включения по сети"
None                     = "Нет"
PatternMatch             = "Соответствие шаблону"
MagicPacket              = "Специальный пакет"
PatternAndMagic          = "Соответствие шаблону И Специальный пакет"
GreenEthernet            = "Зеленый Ethernet"
WakeOnPtn                = "Включить при совпадении шаблона"
WakeOnMagPkt             = "Включить при срабатывании функции Magic Packet"
ARPOffload               = "Выгрузка протокола ARP"
NsOffload                = "Выгрузка протокола NS"
EEE                      = "Энергосберегающий Ethernet"
HDSplit                  = "Разбиение данных заголовка"
WakeOnLinkUp             = "Включение при соединении"
NumRssQueues             = "Максимальное число очередей RSS"
1Queue                   = "1 очередь"
2Queue                   = "2 очереди"
4Queue                   = "4 очереди"
IPSecv2                  = "Выгрузка IPsec"
AH                       = "Авторизация заголовка включена"
ESP                      = "Функция ESP включена"
AHESP                    = "Авторизация заголовка и функция ESP включены"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Slovak
[Strings.041b]
Killer                  = "Killer"
AutoDetect               = "Automatické vyjednávanie"
SpeedDuplex              = "Rýchlosť a duplexný režim"
10Mb-Half-Duplex         = "10 Mbps polovične duplexný"
10Mb-Full-Duplex         = "10 Mbps plne duplexný"
100Mb-Half-Duplex        = "100 Mbps polovične duplexný"
100Mb-Full-Duplex        = "100 Mbps plne duplexný"
1000Mb-Full-Duplex       = "1,0 Gbps plne duplexný"
2.5Gb-Full-Duplex        = "2,5 Gbps plne duplexný"
NetworkAddress           = "Sieťová adresa"
IPChksumOffv4            = "Kontrolný súčet zníženej záťaže IPv4"
TCPChksumOffv4           = "Kontrolný súčet zníženej záťaže TCP (IPv4)"
UDPChksumOffv4           = "Kontrolný súčet zníženej záťaže UDP (IPv4)"
TCPChksumOffv6           = "Kontrolný súčet zníženej záťaže TCP (IPv6)"
UDPChksumOffv6           = "Kontrolný súčet zníženej záťaže UDP (IPv6)"
Enabled                  = "Aktivovaný"
Disabled                 = "Deaktivovaný"
TxEnabled                = "Tx aktivovaný"
RxEnabled                = "Rx aktivovaný"
RxTxEnabled              = "Rx a Tx aktivované"
LSOv4                    = "Veľká odoslaná znížená záťaž (IPv4)"
LSOv2v4                  = "Veľká odoslaná znížená záťaž v2 (IPv4)"
LSOv2v6                  = "Veľká odoslaná znížená záťaž v2 (IPv6)"
FlowControl              = "Ovládanie toku"
PriorityVLAN             = "Priorita a VLAN"
PriorityVLANDisabled     = "Priorita a VLAN sú deaktivované"
PriorityVLANEnabled      = "Priorita a VLAN sú aktivované"
InterruptModeration      = "Prerušiť moderovanie"
ReceiveBuffers           = "Medzipamäte pre príjem"
TransmitBuffers          = "Medzipamäte pre prenos"
AutoDisableGigabit       = "Automaticky zablokovať Gigabit"
AutoLinkDownPhyOff       = "Automaticky zablokovať PHY"
BatteryRe-Link           = "Opätovne spojiť, batéria"
AcBatteryRe-Link         = "Opätovne spojiť, batéria alebo striedavý prúd"
Battery                  = "Aktivovaný, batéria"
AcBattery                = "Aktivovaný, batéria alebo striedavý prúd"
JumboFrame               = "Jumbo rámček"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Vypnutie po pripojení k LAN"
AutoLinkDownPcieMacOff   = "Automaticky zablokovať PCIe"
RSS                      = "Prijať bočnú zmenu mierky"
AutoCrossoverDet         = "Automatické zistenie hraničnej hodnoty"
PriorityEnabled          = "Priorita je aktivovaná"
VLANEnabled              = "VLAN je aktivovaná"
10MbFirst                = "Najprv 10 Mbps"
100MbFirst               = "Najprv 100 Mbps"
WolShutdownLinkSpeed     = "Rýchlosť WOL a vypnutia spojenia"
NotSpeedDown             = "Neznížiť rýchlosť"
WolCap                   = "Možnosti po pripojení k LAN"
None                     = "Žiadne"
PatternMatch             = "Zhoda vzorky"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Zhoda vzorky a Magic Packet"
GreenEthernet            = "Zelený Ethernet"
WakeOnPtn                = "Funkcia Wake on pattern match (Zapnúť funkciu Zhoda vzoru)"
WakeOnMagPkt             = "Nástroj Wake on Magic Packet (Zapnúť aplikáciu Kúzelný balík)"
ARPOffload               = "Nepriame zavádzanie ARP"
NsOffload                = "Nepriame zavádzanie NS"
EEE                      = "Energeticky účinný Ethernet"
HDSplit                  = "Rozdeliť údaje záhlavia"
WakeOnLinkUp             = "Funkcia Wake On Link Up (Zapnúť linku)"
NumRssQueues             = "Maximálny počet frontov RSS"
1Queue                   = "1 front "
2Queue                   = "2 fronty"
4Queue                   = "4 fronty"
IPSecv2                  = "Nepriame zavádzanie IPsec"
AH                       = "Aktivované overenia záhlavia "
ESP                      = "Aktivované ESP"
AHESP                    = "Aktivované overenia záhlavia a ESP "
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Slovenian
[Strings.0424]
Killer                  = "Killer"
AutoDetect               = "Samopogajanje"
SpeedDuplex              = "Hitrost in dupleks"
10Mb-Half-Duplex         = "10 Mb/s Polovični dupleks"
10Mb-Full-Duplex         = "10 Mb/s Polni dupleks"
100Mb-Half-Duplex        = "100 Mb/s Polovični dupleks"
100Mb-Full-Duplex        = "100 Mb/s Polni dupleks"
1000Mb-Full-Duplex       = "1.0 Gb/s Polni dupleks"
2.5Gb-Full-Duplex        = "2.5 Gb/s Polni dupleks"
NetworkAddress           = "Omrežni naslov"
IPChksumOffv4            = "IPv4 Razbremenitev kontrolne vsote"
TCPChksumOffv4           = "TCP Razbremenitev kontrolne vsote (IPv4)"
UDPChksumOffv4           = "UDP Razbremenitev kontrolne vsote (IPv4)"
TCPChksumOffv6           = "TCP Razbremenitev kontrolne vsote (IPv6)"
UDPChksumOffv6           = "UDP Razbremenitev kontrolne vsote (IPv6)"
Enabled                  = "Omogočeno"
Disabled                 = "Onemogočeno"
TxEnabled                = "Tx Omogočeno"
RxEnabled                = "Rx Omogočeno"
RxTxEnabled              = "Rx in Tx omogočeno"
LSOv4                    = "Razbremenitev velikega prenosa (IPv4)"
LSOv2v4                  = "Razbremenitev velikega prenosa v2 (IPv4)"
LSOv2v6                  = "Razbremenitev velikega prenosa v2 (IPv6)"
FlowControl              = "Kontrola pretoka"
PriorityVLAN             = "Prednost in VLAN"
PriorityVLANDisabled     = "Prednost in VLAN onemogočena"
PriorityVLANEnabled      = "Prednost in VLAN omogočena"
InterruptModeration      = "Prekinjena moderacija"
ReceiveBuffers           = "Prejmi medpomnilnike"
TransmitBuffers          = "Prenesi medpomnilnike"
AutoDisableGigabit       = "Samodejno onemogočenje Gigabit"
AutoLinkDownPhyOff       = "Samodejno onemogočenje PHY"
BatteryRe-Link           = "Po-povezava, baterija"
AcBatteryRe-Link         = "Po-povezava, baterija ali AC"
Battery                  = "Omogočeno, baterija"
AcBattery                = "Omogočeno, baterija ali AC"
JumboFrame               = "Jumbo okvir"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Zaustavitev Bujenje-na-Lan"
AutoLinkDownPcieMacOff   = "Samodejno onemogočenje PCIe"
RSS                      = "Sprejmi stransko merilo"
AutoCrossoverDet         = "Samodejno križno zaznavanje"
PriorityEnabled          = "Prednost omogočena"
VLANEnabled              = "VLAN omogočen"
10MbFirst                = "10 Mb/s Najprej"
100MbFirst               = "100 Mb/s Najprej"
WolShutdownLinkSpeed     = "Hitrost zaustavitve povezave in WOL"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Zeleni Ethernet"
WakeOnPtn                = "Zbudi ob enakem vzorcu"
WakeOnMagPkt             = "Zbudi ob paketu Magic"
ARPOffload               = "Prelaganje ARP"
NsOffload                = "Prelaganje NS"
EEE                      = "Energijsko učinkovit ethernet"
HDSplit                  = "Delitev podatkov v glavi"
WakeOnLinkUp             = "Zbudi ob vzpostavitvi povezave"
NumRssQueues             = "Največje število čakalnih vrst RSS"
1Queue                   = "1 čakalna vrsta"
2Queue                   = "2 čakalni vrsti"
4Queue                   = "4 čakalne vrste"
IPSecv2                  = "Prelaganje IPsec"
AH                       = "Glava za overjanje omogočena"
ESP                      = "ESP omogočen"
AHESP                    = "Glava za overjanje in ESP omogočena"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Spanish
[Strings.040A]
Killer                  = "Killer"
AutoDetect               = "Negociación automática"
SpeedDuplex              = "Velocidad y Dúplex"
10Mb-Half-Duplex         = "10 Mbps Half Dúplex"
10Mb-Full-Duplex         = "10 Mbps Full Dúplex"
100Mb-Half-Duplex        = "100 Mbps Half Dúplex"
100Mb-Full-Duplex        = "100 Mbps Full Dúplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Dúplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Dúplex"
NetworkAddress           = "Dirección de red"
IPChksumOffv4            = "Descarga de suma de comprobación IPv4"
TCPChksumOffv4           = "Descarga de suma de comprobación TCP (IPv4)"
UDPChksumOffv4           = "Descarga de suma de comprobación UDP (IPv4)"
TCPChksumOffv6           = "Descarga de suma de comprobación TCP (IPv6)"
UDPChksumOffv6           = "Descarga de suma de comprobación UDP (IPv6)"
Enabled                  = "Activado"
Disabled                 = "Desactivado"
TxEnabled                = "Tx activada"
RxEnabled                = "Rx activada"
RxTxEnabled              = "Rx y Tx activado"
LSOv4                    = "Descarga de gran envío (IPv4)"
LSOv2v4                  = "Descarga de gran envío v2 (IPv4)"
LSOv2v6                  = "Descarga de gran envío v2 (IPv6)"
FlowControl              = "Control de flujo"
PriorityVLAN             = "Prioridad y VLAN"
PriorityVLANDisabled     = "Prioridad y VLAN desactivada"
PriorityVLANEnabled      = "Prioridad y VLAN activada"
InterruptModeration      = "Moderación de interrupción"
ReceiveBuffers           = "Búferes de recepción"
TransmitBuffers          = "Búferes de transmisión"
AutoDisableGigabit       = "Desactivar Gigabit automáticamente"
AutoLinkDownPhyOff       = "Desactivar PHY automáticamente"
BatteryRe-Link           = "Reenlazar, batería"
AcBatteryRe-Link         = "Reenlazar, batería o AC"
Battery                  = "Activado, batería"
AcBattery                = "Activado, batería o AC"
JumboFrame               = "Trama Jumbo"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Activación con LAN de apagado"
AutoLinkDownPcieMacOff   = "Desactivar automáticamente PCIe"
RSS                      = "Escalado lateral de recepción"
AutoCrossoverDet         = "Detección automática de cruce"
PriorityEnabled          = "Prioridad habilitada"
VLANEnabled              = "VLAN activada"
10MbFirst                = "10 Mbps Primero"
100MbFirst               = "100 Mbps Primero"
WolShutdownLinkSpeed     = "Velocidad de enlace WOL y Apagado"
NotSpeedDown             = "Sin reducción de velocidad"
WolCap                   = "Funciones Wake-On-Lan"
None                     = "Ninguno"
PatternMatch             = "Comparar patrón"
MagicPacket              = "Paquete mágico"
PatternAndMagic          = "Comparar patrón y paquete mágico"
GreenEthernet            = "Ethernet ecológico"
WakeOnPtn                = "Reactivar en coincidencia de patrones"
WakeOnMagPkt             = "Reactivar en Magic Packet"
ARPOffload               = "Descarga ARP"
NsOffload                = "Descarga NS"
EEE                      = "Ethernet de consumo eficiente de energía"
HDSplit                  = "División de datos de encabezado"
WakeOnLinkUp             = "Wake on Link (Reactivar en vínculo)"
NumRssQueues             = "Número máximo de colas de RSS"
1Queue                   = "1 Cola"
2Queue                   = "2 Colas"
4Queue                   = "4 Colas"
IPSecv2                  = "Descarga de IPsec"
AH                       = "Encabezado de autenticación habilitado"
ESP                      = "ESP habilitado"
AHESP                    = "Encabezado de autenticación y ESP habilitados"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Swedish
[Strings.041D]
Killer                  = "Killer"
AutoDetect               = "Automatisk förhandling"
SpeedDuplex              = "Hastighet & duplex"
10Mb-Half-Duplex         = "10 Mbps Halv duplex"
10Mb-Full-Duplex         = "10 Mbps Full duplex"
100Mb-Half-Duplex        = "100 Mbps Halv duplex"
100Mb-Full-Duplex        = "100 Mbps Full duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Nätverksadress"
IPChksumOffv4            = "IPv4 Avbelasta kontrollsumma"
TCPChksumOffv4           = "TCP avbelasta kontrollsumma (IPv4)"
UDPChksumOffv4           = "UDP avbelasta kontrollsumma (IPv4)"
TCPChksumOffv6           = "TCP avbelasta kontrollsumma (IPv6)"
UDPChksumOffv6           = "UDP avbelasta kontrollsumma (IPv6)"
Enabled                  = "Aktiverad"
Disabled                 = "Inaktiverad"
TxEnabled                = "Tx aktiverad"
RxEnabled                = "Rx aktiverad"
RxTxEnabled              = "Rx & Tx aktiverad"
LSOv4                    = "Avbelastning för stor överföring (IPv4)"
LSOv2v4                  = "Avbelastning för stor överföring v2 (IPv4)"
LSOv2v6                  = "Avbelastning för stor överföring v2 (IPv6)"
FlowControl              = "Flödeskontroll"
PriorityVLAN             = "Prioritet & VLAN"
PriorityVLANDisabled     = "Prioritet & VLAN inaktiverad"
PriorityVLANEnabled      = "Prioritet & VLAN aktiverad"
InterruptModeration      = "Gruppering av avbrott"
ReceiveBuffers           = "Mottagningsbuffertar"
TransmitBuffers          = "Överföringsbuffertar"
AutoDisableGigabit       = "Automatisk inaktivering av gigabit"
AutoLinkDownPhyOff       = "Automatisk inaktivering av PHY"
BatteryRe-Link           = "Länka om, batteri"
AcBatteryRe-Link         = "Länka om, batteri eller AC"
Battery                  = "Aktiverad, batteri"
AcBattery                = "Aktiverad, batteri eller AC"
JumboFrame               = "Jumboram"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Avsluta Wake-on-LAN"
AutoLinkDownPcieMacOff   = "Automatisk inaktivering av PCIe"
RSS                      = "Ta emot sidskalning"
AutoCrossoverDet         = "Automatisk crossover-identifiering"
PriorityEnabled          = "Prioritet aktiverad"
VLANEnabled              = "VLAN aktiverat"
10MbFirst                = "10 Mbps först"
100MbFirst               = "100 Mbps först"
WolShutdownLinkSpeed     = "WOL och länkhastighet vid avslutning"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Grönt Ethernet"
WakeOnPtn                = "Vakna vid matchat mönster"
WakeOnMagPkt             = "Vakna vid Magiskt paket"
ARPOffload               = "ARP-avlastning"
NsOffload                = "NS-avlastning"
EEE                      = "Energieffektivt Ethernet"
HDSplit                  = "Delning av rubrikdata"
WakeOnLinkUp             = "Vakna vid upplänkning"
NumRssQueues             = "Maximalt antal RSS-köer"
1Queue                   = "1 Kö"
2Queue                   = "2 Köer"
4Queue                   = "4 Köer"
IPSecv2                  = "IPsec-avlastning"
AH                       = "Auth rubrik aktiverad"
ESP                      = "ESP aktiverat"
AHESP                    = "Auth rubrik och ESP aktiverat"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Thai
[Strings.041E]
Killer                  = "Killer"
AutoDetect               = "การปรับอัตโนมัติ"
SpeedDuplex              = "ความเร็ว & ดูเพล็กซ์"
10Mb-Half-Duplex         = "10 Mbps ฮาล์ฟดูเพล็กซ์"
10Mb-Full-Duplex         = "10 Mbps ฟุลดูเพล็กซ์"
100Mb-Half-Duplex        = "100 Mbps ฮาล์ฟดูเพล็กซ์"
100Mb-Full-Duplex        = "100 Mbps ฟุลดูเพล็กซ์"
1000Mb-Full-Duplex       = "1.0 Gbps ฟุลดูเพล็กซ์"
2.5Gb-Full-Duplex        = "2.5 Gbps ฟุลดูเพล็กซ์"
NetworkAddress           = "เน็ตเวิร์กแอดเดรส"
IPChksumOffv4            = "IPv4 เช็คซัม ออฟโหลด"
TCPChksumOffv4           = "TCP เช็คซัม ออฟโหลด (IPv4)"
UDPChksumOffv4           = "UDP เช็คซัม ออฟโหลด (IPv4)"
TCPChksumOffv6           = "TCP เช็คซัม ออฟโหลด (IPv6)"
UDPChksumOffv6           = "UDP เช็คซัม ออฟโหลด (IPv6)"
Enabled                  = "เปิดทำงาน"
Disabled                 = "ปิดทำงาน"
TxEnabled                = "Tx เปิดทำงาน"
RxEnabled                = "Rx เปิดทำงาน"
RxTxEnabled              = "Rx & Tx เปิดทำงาน"
LSOv4                    = "ส่งออฟโหลดขนาดใหญ่ (IPv4)"
LSOv2v4                  = "ส่งออฟโหลดขนาดใหญ่ v2 (IPv4)"
LSOv2v6                  = "ส่งออฟโหลดขนาดใหญ่ v2 (IPv6)"
FlowControl              = "โฟลว์คอนโทรล"
PriorityVLAN             = "ลำดับความสำคัญ & VLAN "
PriorityVLANDisabled     = "ลำดับความสำคัญ & VLAN ปิดทำงาน"
PriorityVLANEnabled      = "ลำดับความสำคัญ & VLAN เปิดทำงาน"
InterruptModeration      = "ขัดจังหวะโมเดอเรชัน"
ReceiveBuffers           = "บัฟเฟอร์รับ"
TransmitBuffers          = "บัฟเฟอร์รับส่ง"
AutoDisableGigabit       = "ปิดทำงานกิกะบิตอัตโนมัติ"
AutoLinkDownPhyOff       = "ปิดทำงาน PHY อัตโนมัติ"
BatteryRe-Link           = "ลิงค์ใหม่, แบตเตอรี่"
AcBatteryRe-Link         = "ลิงค์ใหม่, แบตเตอรี่หรือ AC"
Battery                  = "เปิดทำงาน, แบตเตอรี่"
AcBattery                = "เปิดทำงาน, แบตเตอรี่หรือ AC"
JumboFrame               = "จัมโบ เฟรม"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "การปลุกแลนหลังปิดเครื่อง"
AutoLinkDownPcieMacOff   = "ปิดทำงาน PCIe อัตโนมัติ"
RSS                      = "การเปลี่ยนขนาดด้านที่ได้รับ"
AutoCrossoverDet         = "การตรวจจับครอสโอเวอร์อัตโนมัติ"
PriorityEnabled          = "ลำดับความสำคัญเปิดทำงาน"
VLANEnabled              = "VLAN เปิดทำงาน"
10MbFirst                = "10 Mbps ก่อน"
100MbFirst               = "100 Mbps ก่อน"
WolShutdownLinkSpeed     = "ความเร็วลิงค์การปลุกแลน & ปิดเครื่อง"
NotSpeedDown             = "ไม่ลดความเร็ว"
WolCap                   = "คุณสมบัติการปลุกแลน"
None                     = "ไม่มี"
PatternMatch             = "รูปแบบตรง"
MagicPacket              = "เมจิก แพคเก็ต"
PatternAndMagic          = "รูปแบบตรง & เมจิก แพคเก็ต"
GreenEthernet            = "กรีนอีเธอร์เน็ต"
WakeOnPtn                = "เปิดเมื่อรูปแบบตรงกัน"
WakeOnMagPkt             = "เปิดด้วย Magic Packet"
ARPOffload               = "ARP ออฟโหลด"
NsOffload                = "NS ออฟโหลด"
EEE                      = "อีเธอร์เน็ตประหยัดพลังงาน"
HDSplit                  = "แยกข้อมูลหัวข้อ"
WakeOnLinkUp             = "เปิดเมื่อเชื่อมต่อ"
NumRssQueues             = "จำนวนสูงสุดของคิว RSS"
1Queue                   = "1 คิว"
2Queue                   = "2 คิว"
4Queue                   = "4 คิว"
IPSecv2                  = "IPsec ออฟโหลด"
AH                       = "เปิดใช้งานหัวเรื่องการรับรอง"
ESP                      = "เปิดใช้งาน ESP"
AHESP                    = "เปิดใช้งานหัวเรื่องการรับรองและ ESP"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Turkish
[Strings.041F]
Killer                  = "Killer"
AutoDetect               = "Otomatik Görüşme"
SpeedDuplex              = "Hız & İkili"
10Mb-Half-Duplex         = "10 Mbps Yarım İkili"
10Mb-Full-Duplex         = "10 Mbps Tam İkili"
100Mb-Half-Duplex        = "100 Mbps Yarım İkili"
100Mb-Full-Duplex        = "100 Mbps Tam İkili"
1000Mb-Full-Duplex       = "1.0 Gbps Tam İkili"
2.5Gb-Full-Duplex        = "2.5 Gbps Tam İkili"
NetworkAddress           = "Ağ Adresi"
IPChksumOffv4            = "IPv4 Boşaltmayı Sağla"
TCPChksumOffv4           = "TCP Boşaltmayı Sağla (IPv4)"
UDPChksumOffv4           = "UDP Boşaltmayı Sağla (IPv4)"
TCPChksumOffv6           = "TCP Boşaltmayı Sağla (IPv6)"
UDPChksumOffv6           = "UDP Boşaltmayı Sağla (IPv6)"
Enabled                  = "Etkinleştirildi"
Disabled                 = "Devre Dışı Bırakıldı"
TxEnabled                = "Tx Etkinleştirildi"
RxEnabled                = "Rx Etkinleştirildi"
RxTxEnabled              = "Rx & Tx Etkinleştirildi"
LSOv4                    = "Boşaltmayı Geniş Gönder (IPv4)"
LSOv2v4                  = "Boşaltmayı Geniş Gönder v2 (IPv4)"
LSOv2v6                  = "Boşaltmayı Geniş Gönder v2 (IPv6)"
FlowControl              = "Akış Denetimi"
PriorityVLAN             = "Öncelik & VLAN"
PriorityVLANDisabled     = "Öncelik & VLAN Devre Dışı Bırakıldı"
PriorityVLANEnabled      = "Öncelik & VLAN Etkinleştirildi"
InterruptModeration      = "Hafifletmeyi Kes"
ReceiveBuffers           = "Arabellekleri Al"
TransmitBuffers          = "Arabellekleri İlet"
AutoDisableGigabit       = "Gigabit’i (PowerSaving) Otomatik Olarak Devredışı Bırak"
AutoLinkDownPhyOff       = "PHY’yi (PowerSaving) Otomatik Olarak Devredışı Bırak"
BatteryRe-Link           = "Yeniden Bağla, Pil"
AcBatteryRe-Link         = "Yeniden Bağla, Pil veya AC"
Battery                  = "Etkinleştirildi, Pil"
AcBattery                = "Etkinleştirildi, Pil veya AC"
JumboFrame               = "Jumbo Çerçeve"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Yerel Ağ Üzerinden Kapat"
AutoLinkDownPcieMacOff   = "PCIe’yi (PowerSaving) Otomatik Olarak Devredışı Bırak"
RSS                      = "Yan Ölçüyü Al"
AutoCrossoverDet         = "Otomatik Geçiş Algılama"
PriorityEnabled          = "Öncelik Etkinleştirildi"
VLANEnabled              = "VLAN Etkinleştirildi"
10MbFirst                = "10 Mbps Önce"
100MbFirst               = "100 Mbps Önce"
WolShutdownLinkSpeed     = "WOL & Kapatma Bağlantı Hızı"
NotSpeedDown             = "Yavaşlatma Değil"
WolCap                   = "Lan’da Uyan Özellikleri"
None                     = "Yok"
PatternMatch             = "Örnek Eşleşmesi"
MagicPacket              = "Sihirli Paket"
PatternAndMagic          = "Örnek Eşleşmesi & Sihirli Paket"
GreenEthernet            = "Yeşil Ethernet"
WakeOnPtn                = "Desen eşleştirme uyanması"
WakeOnMagPkt             = "Sihirli Paket Eşleştirme Uyanması"
ARPOffload               = "ARP Yük Boşaltma"
NsOffload                = "NS Yük Boşaltma"
EEE                      = "Enerji Tasarruflu Ethernet"
HDSplit                  = "Üstbilgi Verilerini Bölme"
WakeOnLinkUp             = "Bağlantı Uyanması"
NumRssQueues             = "En Fazla RSS Sırası Sayısı"
1Queue                   = "1 Sıra"
2Queue                   = "2 Sıra"
4Queue                   = "4 Sıra"
IPSecv2                  = "IPsec Yük Boşaltması"
AH                       = "Kimlik Doğrulama Üstbilgisi Etkin"
ESP                      = "ESP Etkin"
AHESP                    = "Kimlik Doğrulama & ESP Etkin"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

;Ukrainian
[Strings.0422]
Killer                  = "Killer"
AutoDetect               = "Автоматичне узгодження"
SpeedDuplex              = "Швидкість і дуплексний режим"
10Mb-Half-Duplex         = "10 Мб/с — півдуплексний"
10Mb-Full-Duplex         = "10 Мб/с — повнодуплексний"
100Mb-Half-Duplex        = "100 Мб/с — півдуплексний"
100Mb-Full-Duplex        = "100 Мб/с — повнодуплексний"
1000Mb-Full-Duplex       = "1,0 Гб/с — повнодуплексний"
2.5Gb-Full-Duplex        = "2,5 Гб/с — повнодуплексний"
NetworkAddress           = "Мережева адреса"
IPChksumOffv4            = "Розвантаження контрольної суми IPv4"
TCPChksumOffv4           = "Розвантаження контрольної суми TCP (IPv4)"
UDPChksumOffv4           = "Розвантаження контрольної суми UDP (IPv4)"
TCPChksumOffv6           = "Розвантаження контрольної суми TCP (IPv6)"
UDPChksumOffv6           = "Розвантаження контрольної суми UDP (IPv6)"
Enabled                  = "Увімкнено"
Disabled                 = "Вимкнено"
TxEnabled                = "Tx увімкнено"
RxEnabled                = "Rx увімкнено"
RxTxEnabled              = "Rx і Tx увімкнено"
LSOv4                    = "Розвантаження великого надсилання (IPv4)"
LSOv2v4                  = "Розвантаження великого надсилання верс. 2 (IPv4)"
LSOv2v6                  = "Розвантаження великого надсилання верс. 2 (IPv6)"
FlowControl              = "Регулятор потоку"
PriorityVLAN             = "Пріоритетність та віртуальна локальна мережа"
PriorityVLANDisabled     = "Пріоритетність та віртуальну локальну мережу вимкнено"
PriorityVLANEnabled      = "Пріоритетність та віртуальну локальну мережу увімкнено"
InterruptModeration      = "Переривання черги завершення для керування "
ReceiveBuffers           = "Отримати буфери"
TransmitBuffers          = "Передати буфери"
AutoDisableGigabit       = "Автоматичне вимкнення Gigabit"
AutoLinkDownPhyOff       = "Автоматичне вимкнення фізичної пам'яті"
BatteryRe-Link           = "Повторне з'єднання, акумулятор"
AcBatteryRe-Link         = "Повторне з'єднання, акумулятор або живлення змінного струму"
Battery                  = "Увімкнення, акумулятор"
AcBattery                = "Увімкнено, акумулятор або живлення змінного струму"
JumboFrame               = "Jumbo-кадр"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "Вимкнути дистанційне ввімкнення через локальну мережу"
AutoLinkDownPcieMacOff   = "Автоматичне вимкнення PCIe"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Автоматичне визначення типу кабелю"
PriorityEnabled          = "Пріоритетність увімкнено"
VLANEnabled              = "Віртуальну локальну мережу ввімкнено"
10MbFirst                = "Спершу 10 Мб/с"
100MbFirst               = "Спершу 100 Мб/с"
WolShutdownLinkSpeed     = "Дистанційне ввімкнення через мережу та швидкість з'єднання під час вимкнення"
NotSpeedDown             = "Без зниження швидкості"
WolCap                   = "Функції дистанційного ввімкнення через локальну мережу"
None                     = "Немає"
PatternMatch             = "Збіг послідовності"
MagicPacket              = "Пакети Magic Packett"
PatternAndMagic          = "Збіг послідовності та пакети Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Увімкнення в разі збігу послідовності "
WakeOnMagPkt             = "Увімкнення в разі пакетів Magic Packet"
ARPOffload               = "Розвантаження ARP"
NsOffload                = "Розвантаження NS"
EEE                      = "Energy-Efficient Ethernet"
HDSplit                  = "Поділ даних заголовку"
WakeOnLinkUp             = "Увімкнення після з'єднання"
NumRssQueues             = "Максимальна кількість черг RSS"
1Queue                   = "1 Черга"
2Queue                   = "2 Черги"
4Queue                   = "4 Черги"
IPSecv2                  = "Розвантаження IPsec"
AH                       = "Аутентифікацію заголовку ввімкнено"
ESP                      = "ESP увімкнено"
AHESP                    = "Аутентифікацію заголовку та ESP увімкнено"
S5ARPOffload             = "Розвантаження ARP під час вимкнення"
AdvancedEEE              = "Розширені параметри EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Вибіркове призупинення"
AIPSSelectiveSuspend     = "Розширене енергозбереження в режимі бездіяльності"
SSIdleTimeout            = "Час простоювання під час вибіркового призупинення в режимі бездіяльності"
AIPSSSIdleTimeout        = "Час простоювання AIPS у режимі бездіяльності"
WakeOnLinkChg            = "Увімкнення після зміни з'єднання"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

; Vietnamese
[Strings.042A]
Killer                  = "Killer"
AutoDetect               = "Tự động thỏa thuận"
SpeedDuplex              = "Tốc độ & Song công"
10Mb-Half-Duplex         = "10 Mb/giây bán song công"
10Mb-Full-Duplex         = "10 Mb/giây song công hoàn toàn"
100Mb-Half-Duplex        = "100 Mb/giây bán song công"
100Mb-Full-Duplex        = "100 Mb/giây song công hoàn toàn"
1000Mb-Full-Duplex       = "1 Gb/giây song công hoàn toàn"
2.5Gb-Full-Duplex        = "2.5 Gb/giây song công hoàn toàn"
NetworkAddress           = "Địa chỉ mạng"
IPChksumOffv4            = "Tải kiểm tra tổng IPv4"
TCPChksumOffv4           = "Tải kiểm tra tổng TCP (IPv4)"
UDPChksumOffv4           = "Tải kiểm tra tổng UDP (IPv4)"
TCPChksumOffv6           = "Tải kiểm tra tổng TCP (IPv6)"
UDPChksumOffv6           = "Tải kiểm tra tổng UDP (IPv6)"
Enabled                  = "Bật"
Disabled                 = "Tắt"
TxEnabled                = "Tx bật"
RxEnabled                = "Rx bật"
RxTxEnabled              = "Rx & Tx bật"
LSOv4                    = "Tải nội dung lớn (IPv4)"
LSOv2v4                  = "Tải nội dung lớn v2 (IPv4)"
LSOv2v6                  = "Tải nội dung lớn v2 (IPv6)"
FlowControl              = "Kiểm soát lưu lượng"
PriorityVLAN             = "Ưu tiên & VLAN"
PriorityVLANDisabled     = "Ưu tiên & VLAN tắt"
PriorityVLANEnabled      = "Ưu tiên & VLAN bật"
InterruptModeration      = "Ngắt kiểm soát"
ReceiveBuffers           = "Bộ nhớ đệm nhận"
TransmitBuffers          = "Bộ nhớ đệm gửi"
AutoDisableGigabit       = "Tự động tắt Gigabit (Tiết kiệm năng lượng)"
AutoLinkDownPhyOff       = "Tự động tắt PHY (Tiết kiệm năng lượng)"
BatteryRe-Link           = "Kết nối lại pin"
AcBatteryRe-Link         = "Kết nối lại pin hoặc AC"
Battery                  = "Pin bật"
AcBattery                = "Pin hoặc AC bật"
JumboFrame               = "Khung mở rộng"
4KBMTU                   = "4088 Bytes"
9KBMTU                   = "9014 Bytes"
16KBMTU                  = "16128 Bytes"
S5WakeOnLan              = "LAN hiện hành khi tắt máy"
AutoLinkDownPcieMacOff   = "Tự động tắt PCIe (Tiết kiệm năng lượng)"
RSS                      = "Tỷ lệ bên nhận"
AutoCrossoverDet         = "Tự động bỏ dò tìm"
PriorityEnabled          = "Ưu tiên bật"
VLANEnabled              = "VLAN bật"
10MbFirst                = "10 Mb/giây trước"
100MbFirst               = "100 Mb/giây trước"
WolShutdownLinkSpeed     = "LAN hiện hành & Tắt tốc độ kết nối"
NotSpeedDown             = "Không giảm tốc độ"
WolCap                   = "Chức năng LAN hiện hành"
None                     = "Không áp dụng"
PatternMatch             = "Khớp kiểu"
MagicPacket              = "Gói ảo"
PatternAndMagic          = "Khớp kiểu & Gói ảo"
GreenEthernet            = "Ethernet xanh"
WakeOnPtn                = "Khởi động trùng kiểu"
WakeOnMagPkt             = "Khởi động gói dữ liệu đặc biệt"
ARPOffload               = "Dỡ tải ARP"
NsOffload                = "Giỡ tải NS"
EEE                      = "Ethernet hiệu năng"
HDSplit                  = "Tách dữ liệu tiêu đề"
WakeOnLinkUp             = "Bật kết nối lên"
NumRssQueues             = "Số chuỗi RSS tối đa"
1Queue                   = "1 chuỗi"
2Queue                   = "2 chuỗi"
4Queue                   = "4 chuỗi"
IPSecv2                  = "Dỡ tải IPsec"
AH                       = "Đã bật tiêu đề xác nhận"
ESP                      = "Đã bật ESP"
AHESP                    = "Đã bật tiêu đề xác nhận & ESP"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"
PowerSavingMode          = "Power Saving Mode"
EEEMaxSupportSpeed       = "EEE Max Support Speed"
MSWoLMagPkt              = "Wake on magic packet when system is in the S0ix power state"
RegVlanid                = "VLAN ID"

Killer_LAN_0.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_1.DeviceDesc       = "Killer E2500 Gigabit Ethernet Controller"
Killer_LAN_2.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"
Killer_LAN_3.DeviceDesc       = "Killer E2600 Gigabit Ethernet Controller"


rt640.Service.DispName = "Killer RT640 NT Driver"

DiskDescription      = "Killer Driver Disk 1"

;;;;; InfVer = 2.000

